For 1990-2009 cars

# FRONT ASHTRAY FALLS OUT (INSTALL REVISED ASHTRAY ASSY)

CONDITION: SOME 1991 BUICK SKYLARKS MAY EXPERIENCE INSUFFICIENT RETENTION IN THE FRONT ASHTRAY AND THE ASHTRAY MAY FALL OUT.

CORRECTION: A REVISED ASHTRAY WITH A STRAP TO THE UPPER HOUSING RETAINER IS AVAILABLE FOR AFFECTED VEHICLES.

PART NUMBER INTERIOR COLOR CODE ------------------------- ----------------------

22578110 66I 22577457 20I 22577458 15I 22577459 78I 22577460 67I

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

LABOR OPERATION NUMBER: C2200

LABOR TIME : .2 HOURS

TROUBLE CODE : 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.

COPYRIGHT 1991 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.