For 1990-2009 cars

# OIL FILTER REPLACEMENT PART NUMBER

#### MODELS AFFECTED: 1987 SKYLARKS AND SOMERSETS WITH THE 2.5L L-4 ENGINE (VIN CODE U) AND MANUAL TRANSMISSION

1987 Skylarks and Somersets with manual transmissions use the force balance shaft 2.5L engine. The oil filter is accessed through the oil pan drain plug. This engine and oil filter will have expanded use in 1988.

Customers have commented that this oil filter is not readily available from their Buick dealer. Please ask your Parts Department Manager to stock this filter for your customers. The oil filter part number is 25012305 (AC type PF1072).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.