For 1990-2009 cars

# INCORRECT SEAT BACK CONTROL ALLOWS SEAT BACK/FOLD FORWARD

#### VEHICLES AFFECTED: 1988-1989 N CARLINE

Should comments be received from owners of a 1988 or 1989 N car 4-door sedan model having a front seat that folds forward, as is the case with 2-door coupe seats, it is possible that the 2-door front seat control assembly was installed in the 4-door seat during production.

A new 4-door seat back control assembly can be installed in the seat should the owner wish to have it changed. The following information may be helpful when ordering the correct seat back control assembly from CANSPO.

Usage Control Assembly ----- ---------------- 1988-1989 4 door Passenger: 20718232 Driver: 20718233

1988-1989 2 door Passenger: 16602620 Driver: 16602621

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.