For 1990-2009 cars

# INFO. ON SIR 'DEPOWERED' AIRBAG IDENTIFICATION

REVISION: 11/26/97

THIS BULLETIN IS BEING REVISED TO CORRECT THE LISTED PART NUMBERS. PLEASE DISCARD CORPORATE BULLETIN NUMBER 70-90-05. **********************************************************************

THIS IS A MONTHLY SERVICE NEWSLETTER ARTICLE THIS INFORMATION IS NOT INTENDED TO BE A PUBLISHED BULLETIN

#### SUBJECT: INFORMATION ON SIR "DEPOWERED" AIR BAG IDENTIFICATION

#### MODELS: 1998 BUICK PARK AVENUE/ULTRA

INQUIRIES HAVE BEEN RECEIVED REGARDING THE "DEPOWERED" SIR WHICH WENT INTO PRODUCTION IN MODEL YEAR 1998 AFTER REVISION OF THE FEDERAL REQUIREMENTS INVOLVED. THE NEW AIR BAGS HAVE SPECIFIC PART NUMBERS AND MUST NOT BE SUBSTITUTED FOR PREVIOUSLY INSTALLED AIR BAGS. THE NEW BAGS CAN ONLY BE IDENTIFIED BY THE TAG WHICH APPEARS ON THE BACK SIDE OF THE INFLATOR MODULE.

THE NEW PART NUMBERS ARE AS FOLLOWS AND ARE DEPENDENT UPON THE COLOR OF THE VEHICLE INTERIOR:

NEW OLD 16822922 16758387 16822923 16758388 16822924 16758389 16822925 16758390 16822926 16758391

THIS IS FOR INFORMATION ONLY AND AS STATED, THESE PART NUMBERS SHOULD NOT BE SUBSTITUTED FOR ANY REASON.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1997 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.