For 1990-2009 cars

# SERVICE GUILD: ENGINE OIL LEAK AT REAR MAIN SEAL

#### SUBJECT: ENGINE OIL LEAK AT REAR MAIN SEAL (NEW PART)

#### VEHICLES AFFECTED: 1990 AND PRIOR YEARS A,B,C,E,F,G,H,N,W CARS WITH 900 V6 BUICK ENGINE

A new rear main oil rope seal has been released to service all 900 V6 "Buick" type engines built through the 1990 model year. The part number for the seal is #24501340.

Parts are currently available from CANSPO.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.