For 1990-2009 cars

# SURGE,CHUGGLE, OR FLATNESS PROM SERVICE NEEDED

#### MODELS AFFECTED: 1984 SKYLARKS

Customer driveability comments of surge chuggle or flatness may arise on some 1984 Skylarks equipped with the 2.8L V6 LE2 engine. If normal service procedures (see Service Manual, page 6E1-106) do not correct the conditions, new service PROMs with revised calibrations are now available.

The model applications are:

REVISED SERVICE MODEL PROM ----- ------- 1984 SKYLARK - ALL MODELS (EXCEPT T TYPE) ----------------------------------------- With 2.8L V6 (LE2) and 3 Speed Automatic Transmission (MX1), Federal Emissions System (NA5), and Air Conditioning (C60) 1226983

With 2.8L V6 (LE2) and 3 Speed Automatic Transmission (MX1), Federal Emissions System (NA5), and Without Air Conditioning (C41) 1226990

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.