For 1990-2009 cars

#### Engine Controls Component Location Table

Name | Location | 8A Locator View | Connector End View | Group No.
--- | --- | --- | --- | ---
AutomaticTransaxle | Left Side of Engine Compartment | 201-02, Fig 04 | 202-57 | --
Camshaft Position Sensor | Front Top of Engine | 201-09, Fig 17 | -- | --
Crankshaft Position Sensor | Front Top of Engine | 201-38, Fig 76 | -- | --
Data Link Connector | Left Side of I/P | 201-25, Fig 50 | 202-20 | --
Electronic Ignition | LH Rear of Engine Compartment | 201-10, Fig 19 | 202-52 | --
Engine Cooling Fan Relay | Right Rear of Engine Compartment | 201-02, Fig 03 | 202-53 | --
Engine Compartment Fuse Center | Left Side of Engine Compartment | 201-04, Fig 08 | -- | --
Engine Coolant Temperature (ECT) Sensor | LH Rear of Engine | 201-10, Fig 19 | -- | --
Evaporative Emission Canister Purge Solenoid | Rear of Engine | 201-04, Fig 07 | -- | --
Evaporative Emission Canister Vent Solenoid | Right Front of Engine Compartment | 201-31, Fig 61 | -- | --
Fuel Injectors | Front Top of Engine | 201-09, Fig 17 | -- | --
Fuel Pump Relay | Right Rear of Engine Compartment | 201-02, Fig 03 | 202-53 | --
Fuel Pump Switch/Oil Pressure Sender/Switch | Front Right of Engine | 201-07, Fig 13 | -- | --
Fuel Tank Unit | Under Rear of Vehicle | 201-35, Fig 70 | -- | --
Fuse Block | Left Side of I/P | 201-25, Fig | -- | --
Fuel Tank Vapor Pressure Sensor | Lower Rear of Car-Front of Fuel Tank | 201-33, Fig 66 | -- | --
Fuse Block | LH Lower I/P | 201-27, Fig 53 | -- | --
Idle Air Control Valve | Front of Engine | 201-03, Fig 06 | -- | --
Instrument Panel Cluster | LH Side of I/P | 201-27, Fig 54 | 202-24 | --
Intake Air Temperature (IAT) Sensor | Left Rear of Engine | 201-10, Fig 19 | -- | --
Knock Sensor | LH Rear of Engine | 201-10, Fig 19 | -- | --
Linear Exhaust Gas Recirculation (EGR) Solenoid | RH Front of Engine Compartment | 201-09, Fig 17 | 202-51 | --
Manifold Absolute Pressure (MAP) Sensor | Front Top of Engine | 201-09, Fig 17 | -- | --
Oile Level Switch | Right Rear of Engine | 201-08, Fig 16 | -- | --
Oxygen Sensor | LH Rear of Engine | 201-10, Fig 19 | 202-52 | --
PARK/NEUTRAL Position Switch | Left Side of Engine Compartment | 201-02, Fig 05 | 202-28 | --
Powertrain Conodule (PCM) | RH Front of I/P | 201-23, Fig 45 | 202-29 | --
Rear Heated Oxygen Sensor | Center of Passenger Compartment Under Vehicle | 201-05, Fig 10 | -- | --
Surge Tank Low Coolant Switch | Right Front of Engine Compartment | 201-31, Fig 61 | -- | --
Throttle Position (TP) Sensor | Front of Engine | 201-03, Fig 06 | -- | --