For 1990-2009 cars

Condition | Causes
--- | ---
Foaming, Milky Power Steering Fluid Low Fluid Level Possible Low Pressure |

• | Air is in the fluid.

• | A loss of fluid due to an internal pump leak causing an overflow.

• | Air bubbles in the system are caused by a low fluid level in extremely cold temperatures.

Perform the following steps:

1. Inspect for a leak.
2. Correct the condition.
3. Bleed the system.