For 1990-2009 cars

# C/C RESUME VALVE COVER NEW DESIGN REPLACEMENT COVER

#### MODELS AFFECTED: All Equipped With Resume Cruise Control

A new design resume valve connector cover (illustrated below) is being used in production on all diesel and gasoline AC resume transducers.

If the connector cover is damaged, it can be replaced without replacing the entire resume valve assembly. The connector cover service package part number is 1984405. The new black connector will service all previous resume valve models and is interchangeable with the older design white connector previously supplied in this package.

Usage of the new cover does not change the part number of previously released resume valve assemblies.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.