For 1990-2009 cars

# REVISED W/SHIELD WIPER SWITCH (REVISED SWITCH/LEVER ASSY.)

#### SUBJECT: REVISED WINDSHIELD WIPER/WASHER SWITCH HANDLE (REVISED SWITCH/LEVER ASSEMBLY W/SHORTER STEM)

#### MODELS AFFECTED: 1992 SKYLARK

#### CONDITION:

---------- Some 1992 Skylark operators of vehicles built prior to VIN NC615535 may comment on the position of the windshield wiper/washer handle.

#### CAUSE:

------ The windshield wiper/washer handle may be perceived to be inconvenient due to its length.

#### CORRECTION:

----------- A revised switch/lever assembly with a shorter stem is available to enhance customer satisfaction. Refer to the 1992 Skylark Service Manual page 3F-4 for the proper procedure.

#### Part Number:

1995947 Switch, Windshield Wiper/Washer, With Pulse (CD4) 1995948 Switch, Windshield Wiper/Washer, Without Pulse (exc CD4)

#### PARTS AVAILABILITY:

Parts are currently available from GMSPO.

#### WARRANTY INFORMATION:

Labor Operation No.: T1820 Labor Time: 0.4 Hrs. Trouble Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.