RADIO TRIM PLATE REMOVAL SPECIAL TOOL AVAILABLE. Buick Somerset 1985

For 1990-2009 cars

# RADIO TRIM PLATE REMOVAL SPECIAL TOOL AVAILABLE

#### VEHICLES AFFECTED: 1985 Calais Without Auto-Calculator

Borroughs Tools and Equipment has made available a special tool, BT 8517, which simplifies removal of the lower ashtray housing. The lower ashtray housing must be removed to remove the radio trim plate on a 1985 Calais not equipped with an Auto-Calculator.

Service Procedure

1. Open the lower ashtray housing and remove ashtray.

2. Push lower ashtray housing in until front of lower housing is approximately 38-51mm (1.5-2.0 inches) from trim plate.

3. Insert BT 8517 into opening as shown in Figure 1.

4. While pressing on tool, push lower housing outward until it is free of the trim plate.

5. To reinstall lower housing, reinstall BT 8517 as shown in Figure 1.

6. Position lower housing into the tracks of the upper housing. Depress the tabs slightly so that the lower housing enters the upper housing easily and push lower housing fully forward.

7. Remove tool.

The tool can be ordered from

Jobborn Manufacturing (1975) Ltd. 97 Frid Street Hamilton, Ont., L8P 4K3 Phone: 416-522-5223

Tool will be available March 15,1985.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.