INOP. ELEC. QUARTZ SPEEDO ADAPTER TO WIRE HARNESS. Buick Somerset 1986

For 1990-2009 cars

# INOP. ELEC. QUARTZ SPEEDO ADAPTER TO WIRE HARNESS

#### VEHICLES AFFECTED: 1986 CALAIS WITH OPTION U21

Some early production 1986 Calais models equipped with the analog instrument cluster and option U21 may experience an intermittent cruise control disengagement and/or inoperative speedometer. This condition may be caused by a poor connection between the cluster printed circuit and wiring harness connector. To correct this condition, it may be necessary to install adapter part no. 22532030 at the wiring harness connector. Refer to Fig. 1. Follow procedures outlined in Sectiori 8C2-9 of the 1986 Chassis Service Manual for removal and reinstallation of the instrument panel cluster.

All vehicles built after October 31, 1985 utilize this adapter, therefore requiring no installation.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.