VIBRATION ON ACCELERATION TRANSAXLE STRUT. Buick Somerset 1985

For 1990-2009 cars

# VIBRATION ON ACCELERATION TRANSAXLE STRUT

#### VEHICLES AFFECTED: 1985 'N' Series Vehicles

The automatic transaxle strut shown in Figure 1 is for anti-vibration use on Pontiac and early Buick 'N' series vehicles only. The strut is designed for use with certain weight distribution factors.

The strut is NOT to be installed on the Oldsmobile Calais. Installation of the strut on the Calais may cause a slight vibration when accelerating from a stop.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.