LOCKING WIRE WHEEL COVERS 1986 MODELS WITH OPTION N91. Buick Somerset 1986

For 1990-2009 cars

# LOCKING WIRE WHEEL COVERS 1986 MODELS WITH OPTION N91

#### MODELS AFFECTED: ALL 1986 MODELS

The custom locking wire wheel cover package (Option N91) is shipped in the trunk comparment.

At the time of delivery of a new vehicle by the carrier, the contents of the package containing Option N91 are to be inspected for missing or incorrect parts. The contents of Option N91 should include:

Four (4) Wire Wheel Covers with Lock Nuts/Bolts Four (4) Lock Brackets Four (4) Medallions One (1) Lock Key Wrench One (1) I.D./Registration Card and Instructions Twelve (12) Flange Lug Nuts (Installed on Wheels)

#### NOTICE: Some 1986 Skylark, Somerset and Century models have only (6) six flanged lug nuts installed on rear wheels and two (2) lock brackets in the trunk package. 1986 Electra and Riviera trunk package also contains twelve (12) anti-rotation clips.

Any discrepancies are to be noted on the delivery receipt and a transportation claim is to be filled out for any missing or incorrect parts.

#### Replacement of Missing, Incorrect or Lost Parts

Lock key wrenches and/or I.D. Registration Cards are available from Norris Industries, Inc.

A. Lock key wrench missing upon delivery of vehicle from factory or lost at dealership after delivery:

Send I.D./Registration Card along with a check in the amount of $8.00 for the replacement lock, key wrench to Norris Industries, Inc.

B. I.D./Registration Card missing:

Provide Norris Industries, Inc. with the color of the stripe and/or letter stamped in the shaft on the lock key wrench. A new color coordinated I.D./Registration Card will be forwarded to the dealership.

C. Lock key wrench does not fit lock bolt or nut:

Send lock key wrench and I.D./Registration Card to Norris Industries, Inc. with a letter indicating the color of the lock bolt or nut in the center of the locking wire wheel cover. The proper lock key wrench and I.D./Registration Card will be returned to the dealership.

D. I.D./Registration Card and "T" shaped lock key wrench both missing:

Provide the color of the lock bolt/nut in the center of the wire wheel cover, along with a check in the amount of $8.00 made payable to Norris Industries, Inc.

#### Parts Ordering

All requests for lock key wrenches and I.D./Registration Cards must be made on dealership stationary to:

Norris Industries, Inc. Automotive Trim Division 39600 Orchard Hill Place Novi, MI 48050

When the vehicle is being made ready for delivery, the lock brackets are to be installed prior to installation of the wire wheel cover and medallions.

1. Raise vehicle with lift equipment.

2. Remove three (3) lug nuts from each wheel for lock bracket installation. Somerset and second type Century.

#### NOTICE: 1986 Skylark, Somerset and Second Type Century front-wheel covers are retained by the drive axles; therefore, they do not require lock brackets.

3. Place lock bracket on lug nut studs.

4. Install three (3) special lug muts on each wheel to retain lock bracket and torque to specifications. LOOSE CONDITION OF LOCK BRACKET WILL BE NORMAL. WHEN LUG NUTS ARE SEATED, FRONT WHEEL STUDS WILL HAVE A RECESSED APPEARANCE, WHICH IS NORMAL.

5. Install adapter or anit-rotation clips if required.

6. Align valve notch in wire wheel cover with valve stem on wheel. For center retention covers (Electra, LeSabre, Riviera, second type Skylark and Somerset, and second type Century) place cover on wheel by hand only. DO NOT USE A HAMMER TO INSTALL COVERS. A rubber mallet may be required to install covers that have an outer rim retention design.

7. Tighten lock nut or bolt by turning lock key wrench clockwise. This will secure the wire wheel cover.

8. Snap in center medallion.

9. Install the Wire Wheel Cover Removal Instruction label as required.

10. The lock key wrench is to be placed in the glove boz or trunk compartment as explained in the installation instructions. Place the I.D./Registration Card in the glove box.

The procedure for removal and installation is to be explained to the owner prior to delivery.

Other missing or incorrect part(s) such as locking wire wheel cover(s), lock bracket(s), medallion(s) and special lock nuts or bolt(s) are available through GMWDD.

1986 BUICK WIRE WHEEL COVERS

Skyhawk Somerset Century Century Century & Skylark Design I Design I Design II w/JA1 w/JA2/JA8 w/JA1 13" 13" 14" 14" 14" -------- --------- -------- --------- ---------- Cover Package (Complete) 999233 999233 997788 998547 999230

Cover Asm 22533083 22533083 25511220 25511220 25525823

Cup & Medallion 22532104 22532104 25512648 25512648 22532104 (Emblem)

Bolt Circle l00mm 100mm l00mm 115mm 110mm

Lock Bracket 22531453 22531453 22515623 22526979 22531453 Assy

Adapter or Anti Rotation Clips

Wheel Nut 1617075 1617075 1617075 1617075 1617075

Bolt/Nut Nut Nut Bolt Bolt Nut Pattern Scallop Scallop

Red 22531448 22531448 14035631(A) 14035631(A) 22531297 Green 22531449 22531449 14035632(B) 14035632(B) 22531298 Blue Gold or Yellow 22531452 22531452 14035634(H) 14035634(H) 22531301 Orange Dk Brown 14035633(C) 14035633(C) Black 22531450 22531450 14035635(L) 14035635(L) 22531299 Silver 22531451 22531451 22531300 Tan Gray LeSabre & Century Regal LeSabre Electra Design II Estate w/JA2/JA8 Wagon 14" 14" 14" 15" --------- ------ ------- ---------

Cover Package 997093 998568 997092 (Complete) 999231 25506533 25523352 25506534 Cover Asm 25525823 25506531 25515955 25506530 Cup & Medallion 22532104 (Emblem) 4.75in. 115mm 5.00in. Bolt Circle 115mm 25520262 25522565 25520262 Lock Bracket 22522026 Opt.22506313 Assy

Adapter or Anti Rotation Clips 1617075 1617075 22506315 Wheel Nut 1617075 Bolt Nut Bolt Bolt/Nut Nut Pattern 22511949(A) 1630024 22511949(A) Red 22531297 22511950(B) 1630025 22511950(B) Green 22531298 1630026 Blue 2251952(H) 1630027 22511952(H) Gold or Yellow 22531301 1630029 Orange 22511951(C) 1630031 22511951(C) Dk Brown 22511953(L) 1630028 22511953(L) Black 22531299 1630032 Silver 25531300 1630030 Tan 1630033 Gray Electra Riviera

14" 14" ------- ------- Cover Package (Complete) 998568 999232

Cover Asm 25523352 25519335

Cup & Medallion 25515955 25523815 (Emblem)

Bolt Circle 115mm 115mm

Lock Bracket 25522565 25522565 Assy

Adapter or Anti Rotation Clips 25523353

Wheel Nut 1617075 1617075

Bolt/Nut Nut Nut Pattern

Red 1630024 1630024 Green 1630025 1630025 Blue 1630026 1630026 Gold or Yellow 1630027 1630027 Orange 1630029 1630029 Dk Brown 1630031 1630031 Black 1630028 1630028 Silver 1630032 Tan 1630030 Gray

Design has rim type retention Design II has center bolt type retention All parts available through GMWDD

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.