RATTLE FROM FOLDING TOP STOWAG COVER LATCH (REPL. STRIKER). Cadillac Allante 1990

For 1990-2009 cars

# RATTLE FROM FOLDING TOP STOWAG COVER LATCH (REPL. STRIKER)

#### SUBJECT: RATTLE FROM FOLDING TOP STOWAGE COVER LATCH

#### MODELS AFFECTED: 1990-1993 ALLANTES

The folding top stowage cover latch and striker (Figure 1) may rattle when driving over bumps on some 1990-1993 Allantes. The condition is caused by metal-to-metal contact between the striker and latch. To correct the condition replace the striker with a new plastic coated striker, P/N 3543744.

Parts are currently available from GMSPO.

For warranty purposes use Labor Operation B36S8 at .4 hour.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.