INTERMITTENT MESSAGE ON DIC OR ERRATIC A/C OPERATION. Cadillac Allante 1987

For 1990-2009 cars

# INTERMITTENT MESSAGE ON DIC OR ERRATIC A/C OPERATION

#### MODELS AFFECTED: 1986-1989 ELDORADOS AND SEVILLES 1987-1989 ALLANTES

Some 1986-1989 Eldorados and Sevilles and 1987-1989 Allantes may display a "System Problem" message on the Driver Information Center or exhibit erratic A/C operation and set a BCM code B337 in history. To repair a vehicle with this condition replace the programmer with P/N 16137740.

Parts are currently available from GMSPO.

WARRANTY INFORMATION VEHICLE SERIES -------------------- Operation -------------- Operation Description Number C D E J K V --------------------- --------- --------------------- Programmer, R&R D0770 4 .4 .9

Part Group: 9.275

Policy: M (1986 models L (1987-1988 models)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.