WINDSHIELD GLASS REPLACEMENT FOR ALLANTE 1987. Cadillac Allante 1987

For 1990-2009 cars

# WINDSHIELD GLASS REPLACEMENT FOR ALLANTE 1987

#### VEHICLES AFFECTED: 1987 ALLANTE (V)

A new windshield glass assembly P/N 1644586 is available through GMSPO for the 1987 Allante. This assembly consists of the windshield glass, P/N 1635170, mirror plate, P/N 20626174, and a windshield upper reveal moulding, P/N 1635180, which is bonded to the upper edge of the windshield glass.

When servicing the windshield glass, the windshield glass outer seal, P/N 1635173, must also be replaced.

Use the most applicable labour operation from the Canadian Labour Time Guide and claim 3.5 hours.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.