NOISY/BINDING DOOR GLASS OPER. (REPL. DOOR WINDOW MOTOR). Cadillac Allante 1991

For 1990-2009 cars

# NOISY/BINDING DOOR GLASS OPER. (REPL. DOOR WINDOW MOTOR)

====================================================================== REVISION 10/13/93

#### NOTE: THIS BULLETIN WILL NOT BE PUBLISHED. THE REVISED INFORMATION IS PROVIDED ONLY FOR THE TAS DATABASE AND WILL APPEAR ON BULLETIN 310106R, "SERVICE BULLETIN UPDATES".

THIS BULLETIN IS BEING REVISED TO CORRECT THE ALLANTE PART NUMBERS. PART 22073444 SHOULD BE CHANGED TO "LH" AND 22073443 SHOULD BE CHANGED TO "RH". ======================================================================

SOME 1992-1993 ELDORADOS AND SEVILLES AND 1987-1993 ALLANTES MAY EXPERIENCE ONE OR MORE OF THE FOLLOWING CONDITIONS WHEN OPERATING THE SIDE DOOR GLASS:

O DOOR GLASS OPERATION NOISY (CLICKING, POPPING, RATCHETING) O BINDING DOOR GLASS IN UP OR DOWN TRAVEL O INTERMITTENT DOOR GLASS OPERATION O FAILURE OF DOOR GLASS TO OPEN OR CLOSE

THIS CONDITION MAY BE CAUSED BY AN INTERNAL DOOR WINDOW MOTOR SITUATION WHERE THE PLASTIC OUTPUT GEAR TOOTH IS STRESSED BEYOND ITS DESIGN CAPABILITY.

TO CORRECT THIS CONDITION REPLACE ONLY THE DOOR WINDOW MOTOR WITH THE APPROPRIATE PART FROM THE REVISED PARTS LISTED IN THE CHART BELOW. PROCEDURES ARE PROVIDED IN SECTION 10-6 OF THE SERVICE INFORMATION MANUAL.

SERVICE LABOR CARLINE YEAR PART NUMBER OPERATION TIME DIAGNOSIS

ELDORADO 1992-1993 22143946 RH N3314 .5 0-.3 22143945 LH N3315 .5 0-.3

SEVILLE 1992-1993 22143946 RF N3314 .5 0-.3 22143945 LF N3315 .5 0-.3 22143946 RR N3324 .4 0-.3 22143945 LR N3325 .4 0-.3

ALLANTE 1993 22143948 RH N3314 1.4 0-.3 22143947 LH N3315 1.4 0-.3 1987-1992 22073443 RH N3314 1.4 0-.3 22073444 LH N3315 1.4 0-.3

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

FOR WARRANTY PURPOSES USE THE APPROPRIATE LABOR OPERATION LISTED IN THE CHART ABOVE.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1993 CADILLAC MOTOR CAR DIVISION, GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.