For 1990-2009 cars

# Info - September, 2000 Bulletin Summary

Subject: | September, 2000 Bulletin Summary

Models: | 2001 and Prior Passenger Cars and Trucks

The following list is a summary of all the bulletins that were issued in September, 2000. It is intended to let dealerships quickly review the most current bulletins in order to better service their customers. Dealerships will be receiving this type of summary, published as a bulletin, every month.

Bulletin Title | Vehicles Affected | Bulletin Number
--- | --- | ---
Engine
Enhanced Emission Inspection Maintenance Program -- Emissions Diagnostic Manual for OBDII Vehicles | 1996-2000 Passengers Cars and Light Trucks | 00-06-04-033
DEX-COOL® Engine Coolant Information | 2001 and Prior Passenger Cars and Trucks | 00-06-02-006
Service Engine Soon Lamp Illuminates Intermittently, PCM Code P1515 Set (Reprogram PCM) | 2000 Chevrolet Camaro; 2000 Pontiac Firebird With 3.8L Engine | 00-06-04-035
Check Engine Light (MIL) Illuminated, DTC P0411 (Diagnose/Replace Secondary Air Injection Check Valve) | 1997-1999 Cadillac Catera With 3.0L Engine | 00-06-04-032
Fuel Filler Cap Contacts Rear Quarter Panel When Suspended By Tether (Install New Fuel Cap & Tether Assembly) | 2000 Chevrolet Camaro; 2000 Pontiac Firebird | 00-06-04-036
Intermittent Engine Stall (Reprogram Engine Control Unit (ECU)) | 1999-2000 Cadillac Catera | 00-06-04-034
Enhanced Aluminum Engine Component Thread Repair Process | 1993 Cadillac Allante; 1993-2001 Cadillac Eldorado, Seville; 1994-1999 Cadillac DeVille Concours; 1996-2001 Cadillac DeVille; 2000-2001 Cadillac DeVille Touring; 1997-2001 Chevrolet Corvette; 1998-2001 Chevrolet Camaro; 1995-2001 Oldsmobile Aurora (V8); 1999-2001 Oldsmobile Intrigue; 2001 Oldsmobile Aurora (V6); 1998-2001 Pontiac Firebird

With 2.2L, 3.5L, 4.0L or 5.7L Engine

00-06-01-016

Growl/Moan Noise During Sharp Left Turn (Modify Engine Mount Stamping) | 2000 Chevrolet Cavalier; 2000 Pontiac Sunfire With 2.2L Engine | 00-06-01-018
Service Engine Soon (SES) Light On with DTCs P0716 and/or P0717 Set (Repair Input Speed Sensor Wiring at Transaxle Wiring Pass-thru Connector) | 2000-2001 Chevrolet Cavalier, Malibu; 2000-2001 Oldsmobile Alero; 2000-2001 Pontiac Grand Am, Sunfire | 00-06-04-037
Unwanted Switch to Gasoline, Fuel Indicator Lamp (FIL) Inoperative, Cooling Fan Inoperative, Engine Running Hot and/or Overheating (Replace Cooling Fan/CNG Fuse) | 2000 Chevrolet Cavalier With 2.2L Engine and Bi-Fuel | 00-06-04-038
ABS Light On at High Speeds (Above 70 mph or 113 km/h), Code C0237 Set (Install New PCM) | 2000 Chevrolet and GMC S/T Pickup Models With 2.2L Engine and 4L60-E Automatic Transmission | 00-06-04-025A
Exchange Program for 2001 Model Year | 2001 Chevrolet and GMC C/K and G Light Duty Models; 2001 Chevrolet and GMC B7, C6, C7 Medium Duty Models With 8.1L Engine | 99-06-01-002D
Transmissions
Revised DTC Tables for P0716 and P0717 (Section 7 Automatic Transmission) | 1998-2000 Chevrolet and GMC C/K Models and G Van With Hydra-Matic 4L80-E Automatic Transmission | 00-07-30-015
4-3 Downshift Gear Clash, 1-2 Upshift Gear Clash When Cold (Replace Affected Gear, Synchronizer Ring, Synchronizer Assembly and Transmission Fluid) | 1999-2000 Chevrolet Tracker With 5-Speed Manual Transmission | 00-07-29-001
Removal of the PWM Filter from the Spacer Plate-4T40E/4T45E Automatic Transmission | 1998-2000 Chevrolet Cavalier, Malibu; 1998-1999 Oldsmobile Cutlass; 1999-2000 Oldsmobile Alero; 1998-2000 Pontiac Sunfire; 1999-2000 Pontiac Grand Am With 4T40E or 4T45E Automatic Transmission | 00-07-30-016
Clutch Noisy, Slipping or Inoperative (Replace Clutch Release Bearing) | 1990-2000 Chevrolet and GMC C6-7 Conventional Medium Duty Trucks; 1993-2000 Chevrolet and GMC B7 School Buses With Gas or Diesel Engine and Spicer 310 mm Clutch, Valeo 13 inch Clutch, or Midland Lipe Clutch | 00-07-31-001
Body and Accessories
Brush Guard Removal | 1999 Chevrolet Tahoe Utility Models With Off-Road Chassis Package | 00-08-62-002
New Front Air Deflector with Increased Ground Clearance | 1997-2000 Buick Century, Regal; 1998-2000 Oldsmobile Intrigue; 1997-2000 Pontiac Grand Prix | 00-08-63-006
Air/Windnoise Around Front Door (Use All Service Procedures) | 1996-2000 Chevrolet and GMC G Vans | 00-08-64-009
Passenger Seat Easy Entry Feature Does Not Operate Smoothly (Replace Seat Track Adjusters) | 1999-2000 Oldsmobile Alero (Coupe Only); 1999-2000 Pontiac Grand Am (Coupe Only) | 00-08-50-009
Service Manual Update - Addition of DTC B2961 Diagnostics | 2000 Chevrolet and GMC C/K Pickup and Utility Models, S/T Models and M/L Vans 2000 Chevrolet and GMC S/T RHD Models; 2000 Oldsmobile Bravada | 00-08-49-009
Intermittent Operation of Remote Keyless Entry System (Replace Instrument Panel Cluster) | 2000 Chevrolet Impala, Monte Carlo | 00-08-52-004
Engine Mount Crossmember Cracking (Replace Crossmember and Fasteners) | 1993-2000 Chevrolet and GMC B6-7 Medium Duty School Bus Models With 3116/3126 Caterpillar® Diesel Engine | 00-08-61-002
Wind Noise from Body Side Quarter Window (Replace Body Side Quarter Window Assembly) | 1999-2000 Chevrolet and GMC C/K Extended Cab Pickup Trucks (Silverado and Sierra) | 99-08-48-001A
Outside Rear View Mirror Housing Turns Chalky/Dull (Color/Clear Coat Mirror) | 1998-2000 Buick Century, Park Avenue, Regal; 1998-2000 Chevrolet Cavalier, Lumina, Malibu, Metro, Monte Carlo, Prizm, Tracker, Venture; 2000 Chevrolet Impala; 1998-2000 Oldsmobile Intrigue, Silhouette; 1999-2000 Oldsmobile Alero; 1998-2000 Pontiac Bonneville, Grand Am, Sunfire Trans Sport; 1998-2000 Chevrolet and GMC C/K, S/T Models and M/L Van; 1998-2000 Oldsmobile Bravada | 00-08-51-001
General Wind Noise/Windrush (Install Sealer) | 2000 Pontiac Bonneville | 00-08-58-003
Service Manual Update-Revised/Added Sunroof Specifications and Procedures | 2000 Chevrolet and GMC C/K Utility Models | 00-08-67-004
OnStar® System Cellular Antenna Replacement Parts Availability | 1996-2000 Passenger Cars and Trucks | 00-08-46-002
Radio Presets Are Incorrect or Cannot Be Set | 2000-2001 Cadillac DeVille, Seville | 00-08-46-001
General Information
July, 2000 Bulletin Summary | 2001 and Prior Passenger Cars and Trucks | 00-00-89-018
New Electrical Relay Labor Operation Numbers | 2001 and Prior Passenger Cars and Trucks | 00-00-89-019
Cross-line Warranty | 2001 and Prior Passenger Cars and Trucks | 00-00-89-021
September, 2000 Labor Time Guide Updates | 1996-2001 Passenger Cars and Trucks | 00-00-89-020
August, 2000 Bulletin Summary | 2001 and Prior Passenger Cars and Trucks | 00-00-89-022
Brakes
Availability of Rear Wheel Mud Flaps | 1999-2000 Chevrolet and GMC C/K Pickup Models (Silverado and Sierra) | 00-05-23-005
Reduced Brake Pad/Lining Life (Install New Brake Booster Pushrod Lever) | 1997-98 Chevrolet and GMC T-Series Medium Duty Tilt Cab Models With Hydraulic Brakes | 00-05-22-007
HVAC
Production Changes to A/C System Components, Revisions to Reduce Possible Passenger Compartment Hiss Noise and New Charging Guidelines | 1999 Chevrolet Corvette | 99-01-39-006A
RH HVAC Air Outlet Shut-off Door Closes When Blower On High (Install Washer) | 2000 Cadillac DeVille | 00-01-39-001