For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Body Control Module (BCM) | Mounted on the RH A-Pillar, behind the trim panel | -- | --
Data Link Connector (DLC) | Attached to the I/P carrier, to the left of the steering column | -- | --
Electronic Brake/Traction Control Module (EBTCM) | LH front of the engine compartment, mounted to the lower rail | -- | --
Engine Control Module (ECM) | LH front of the engine compartment, in the ECM housing at position 40 | -- | --
Front Side Door Jamb Switch (LH) | Lower LH A-Pillar | -- | --
Front Side Door Jamb Switch (RH) | Lower RH A-Pillar | -- | --
Front Side Door Lock Switch (LH) | Mounted to the inside LH front side door trim panel | -- | --
Front Side Door Lock Switch (RH) | Mounted to the inside RH front side door trim panel | -- | --
Fuse Block | Mounted to the I/P, lower LH side of the steering column | -- | --
Gauge Cluster | LH side of the I/P, just to the left and above the heater & A/C control | -- | --
Horn Relay K63 | Lower I/P, to the RH side of the steering column, on the relay box, at position VI | -- | --
Ignition Switch | Mounted to the ignition lock cylinder | -- | --
Low Beam Relay K131 | Lower I/P, to the RH side of the steering column, on the relay box, at position VIII | -- | --
Park Lamp Relay K130 | Lower I/P, to the RH side of the steering column, on the relay box, at position VII | -- | --
Power Distribution Fuse Block | LH side of the engine compartment, attached to the ECM housing, above the battery | -- | --
Rear Compartment Courtesy Lamp Switch | Attached to the rear compartment lid | -- | --
Rear Side Door Jamb Switch (LH) | Lower LH B-Pillar | -- | --
Rear Side Door Jamb Switch (RH) | Lower RH B-Pillar | -- | --
Remote Control Door Lock Receiver | In the rear compartment, underneath the LH side of the rear window panel trim | -- | --
Theft Deterrent Module | Mounted to the ignition lock cylinder, on the upper RH of the steering column | -- | --
C105 | I/P wiring harness to ECM wiring harness, located at the LH front of the engine compartment | -- | --
C200A | I/P wiring harness to body wiring harness, at the lower LH A-Pillar | -- | --
C200B | I/P wiring harness to body wiring harness, at the lower LH A-Pillar | -- | --
C301 | Body wiring harness to RH courtesy lamp wiring harness, at the base of the RH B-Pillar | -- | --
C302 | Body wiring harness to LH courtesy lamp wiring harness, at the base of the RH B-Pillar | -- | --
C405 | Body wiring harness to rear compartment lid harness | -- | --
C500 | Body wiring harness to LH front side door wiring harness, at the lower LH A-Pillar, near G200 | -- | --
C600 | Body wiring harness to LH front side door wiring harness, at the lower LH A-Pillar, near G200 | -- | --
G103 | Body and I/P wiring harnesses, located at the LH front of the engine compartment, near C102, C105, and C106 | -- | --
G200 | Body wiring harness, at the lower LH A-Pillar, above and to the left of C200 | -- | --
P103 | Lower LH A-Pillar, forward of G200 | -- | --
P108 | LH engine compartment, at the rear of the ECM housing | -- | --
P110 | Rear LH corner of the engine compartment | -- | --
P401 | Lower LH corner of the rear compartment | -- | --
P402 | Upper LH corner of the rear compartment, near the LH taillamp | -- | --
P500 | In the LH front side door, approximately 12 cm (5 in) from the outside remote control rear view mirror switch | -- | --
P600 | In the RH front side door, approximately 25 cm (10 in) from the RH front side door lock switch | -- | --
S103 | Body wiring harness, approximately 27 cm (11 in) from P107 branch break off | -- | --
S104 | Body wiring harness, approximately 83 cm (33 in) from P103, near P107 branch break off | -- | --
S200 | I/P wiring harness, near the data link connector (DLC) | -- | --
S214 | I/p wiring harness, near the data link connector (DLC) branch break off | -- | --
S222 | I/P wiring harness, near G201 branch break off | -- | --
S245 | I/P wiring harness, near the multifunction relay module connector branch break off | -- | --
S250 | I/P wiring harness, near the instrument cluster connector branch break off | -- | --
S264 | Body wiring harness, near G200 branch break off | -- | --
S267 | Body wiring harness, near G200 branch break off | -- | --
S270 | Body wiring harness, approximately 70 cm (27 in) from the console wiring branch break off | -- | --
S308 | Body wiring harness, base of the RH A-Pillar, just under the conduit | -- | --
S309 | Body wiring harness, base of the RH A-Pillar, just under the conduit | -- | --
S317 | Body wiring harness, base of the LH A-Pillar, just under the conduit | -- | --
S319 | Body wiring harness, base of the LH A-Pillar, just under the conduit | -- | --
S502 | LH front side door wiring harness, approximately 26 cm (10 in) from connector | -- | --
S602 | LH front side door wiring harness, approximately 26 cm (10 in) from connector | -- | --