For 1990-2009 cars

Table 1: | Automatic Level Control Sensor
Table 2: | Rear Suspension Leveling Air Compressor Relay K19

#### Automatic Level Control Sensor

Connector Part Information |

• | ZPF 8-1

• | 8-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | A105 | Fused Battery Voltage
B | BRN/WHT | XM900 | Serial Data (Keyword 82)
C | YEL | B25 | Rear Suspension Leveling Relay Control
D | WHT | M101 | Compressor Exhaust Control
E | BLK | F210 | Ground
F | BLU/RED | PA909 | VSS Input
G | BRN/PPL | XY1 | Warning Indicator Control
H | BRN | X300 | Fused Ignition

#### Rear Suspension Leveling Air Compressor Relay K19

Connector Part Information |

• | ZFW 5-20

• | 5-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YEL | B56 | Relay Control Signal
2 | -- | -- | Not Used
3 | BRN | X470 | Fused Ignition
4 | BRN | X43 | Motor ON Signal
5 | RED | A44 | Fused Battery Voltage