For 1990-2009 cars

Table 1: | Adapter Case
Table 2: | Automatic Transmission Control Indicator
Table 3: | Automatic Transmission Range Switch
Table 4: | Automatic Transmission Winter Mode Switch
Table 5: | Main Case
Table 6: | Vehicle Speed Sensor (VSS) Assembly
Table 7: | Transmission Control Module (TCM)

#### Adapter Case

Connector Part Information |

• | ZPF 4-1

• | 4 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/YEL | FB738 | Torque Convertor Clutch (TCC) Solenoid Control Signal
B | BLK/PPL | FY740 | Pressure Control Solenoid (PCS) Valve Signal HI
C | GRY/RED | RA741 | Pressure Control Solenoid (PCS) Valve Signal LO
D | BLU/BLK | PF854 | 12 V TCM Power Relay Signal for Torque Convertor Clutch (TCC) Solenoid Valve

#### Automatic Transmission Control Indicator

Connector Part Information |

• | ZF 12-3

• | 12 Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BLK | F970 | G103
3-4 | -- | -- | Not Used
5 | BRN | X90 | Fused Ignition Feed
6 | GRY/GRN | RU500 | Fused Battery Feed W/ Park Lamp Relay ON
7 | GRY/YEL | RB70 | Dimming Control Signal
8 | BLK/BLU | FP400 | Trans Range Switch Input A
9 | BLK/GRN | FU400 | Trans Range Switch Input B
10 | BLK/YEL | FB400 | Trans Range Switch Input C
11 | GRY | R400 | Trans Range Switch Input P
12 | -- | -- | Not Used

#### Automatic Transmission Range Switch

Connector Part Information |

• | ZPF 8-3

• | 8 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/BLU | FP733 | Trans Range Switch Output A
B | BLK/GRN | FU726 | Trans Range Switch Output B
C | BLK/YEL | FB708 | Trans Range Switch Output C
D | BRN | X756 | Fused Ignition Feed
E | BLK/RED | FA501 | P/N Switch Output To Starter Solenoid
F | WHT/BLK | MF757 | R Signal To Rear View Mirror
G | GRY | R733 | Trans Range Switch Output P
H | BLK/RED | FA500 | Ignition Switch Start (position III) Signal

#### Automatic Transmission Winter Mode Switch

Connector Part Information |

• | ZPM 4-50

• | 4 Way M

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRN | U102 | Winter Mode Switch Output Signal
B | BLK | F960 | G103
C | BRN/GRN | XU100 | 3rd Gear Indicator Control
D | BRN | X14 | Fused Ignition Feed

#### Main Case

Connector Part Information |

• | 12199508

• | ASM 7F M/P 150 (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLU/YEL | PB743 | 2-3 Shift Solenoid Control
B | GRY/BLK | RF745 | Band Apply Solenoid Control
C | BLU/WHT | PM748 | 1-2 and 3-4 Shift Solenoid Control
D | BLU/BLK | PF954 | 12 V TCM Power Relay Signal for Solenoids
E | BRN/GRN | XU716 | TFT Sensor Return
F | BLK/BLU | FP722 | 5 V Reference Signal for TFT Sensor
G | -- | -- | Not Used

#### Vehicle Speed Sensor (VSS) Assembly

Connector Part Information | ZPF 2-2
--- | ---
Pin | Wire Color | Circuit No. | Function
A | BLK/YEL | FB703 | VSS Signal HI
B | BLU/GRN | PU705 | VSS Signal LO

#### Transmission Control Module (TCM)

Connector Part Information |

• | ZF 88-3

• | 88 Way F Bosch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-3 | -- | -- | Not Used
4 | GRY/BLK | RF745 | Band Apply Solenoid Control
5 | GRY/RED | RA741 | Pressure Control Solenoid (PCS) LO Signal
6 | BLK | F819 | Ground to G103
7 | -- | -- | Not Used
8 | BLK/GRN | FU400 | Trans Range Switch Input B
9 | GRY | R400 | Trans Range Switch Input P
10-11 | -- | -- | Not Used
12 | BLU | P100 | Sport Mode Switch Input
13 | GRN | U102 | Winter Mode Switch Input
14 | BLU/GRN | PU714 | VSS LO Signal
15 | BLK | S40 | VSS Shielded Ground
16 | -- | -- | Not Used
17 | BLK/YEL | FB800 | Sport Mode and Transmission Malfunction Indicator Control (2nd design)
18-20 | -- | -- | Not Used
21 | BRN/GRN | XU716 | TFT Sensor Signal Return
22 | BLK/BLU | FP722 | TFT Sensor (5V ref) Signal
23-24 | -- | -- | Not Used
25 | GRY | R133 | Transmission Service Indicator Control (1st design)
25 | -- | -- | Not Used (2nd design)
26 | RED | A828 | Fused Battery Feed
27 | BRN/GRN | XU100 | 3rd Gear Indicator Control
28 | BLK | F836 | Ground to G103
29 | -- | -- | Not Used
30 | BLU/WHT | PM748 | 1-2 and 3-4 Shift Solenoid Control
31 | -- | -- | Not Used
32 | BLK/YEL | FB738 | TCC Solenoid Control
33 | BLU/YEL | PB743 | 2-3 Shift Solenoid Control
34-35 | -- | -- | Not Used
36 | BLK/BLU | FP400 | Trans Range Switch Input A
37 | BLK/YEL | FB709 | Trans Range Switch Input C
38-41 | -- | -- | Not Used
42 | BLK/YEL | FB720 | VSS HI signal
43-48 | -- | -- | Not Used
49 | BRN/GRY | XR888 | CAN Interface LO
50 | BRN/PPL | XY888 | CAN Interface HI
51 | BRN/WHT | XM12 | Serial Data (KW2000)
52 | BLK/PPL | FY740 | Pressure Control Solenoid (PCS) Valve HI Signal
53 | BLU/BLK | PF754 | Power Relay (12V ref) Output
54 | BRN | X837 | Fused Ignition Feed
55-88 | -- | -- | Not Used