For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
A/C Compressor Refrigerant Pressure Switch | LH front of the engine compartment, mounted in the A/C compressor/condensor hose, below the A/C load switch | Cooling System Component Views in Engine Cooling | Cooling System Connector End Views in Engine Cooling
Auxiliary Engine Coolant Fan #1 | Front of the LH side of the radiator | Cooling System Component Views in Engine Cooling | Cooling System Connector End Views in Engine Cooling
Auxiliary Engine Coolant Fan #2 | Front of the RH side of the radiator | Cooling System Component Views in Engine Cooling | Cooling System Connector End Views in Engine Cooling
Auxiliary Water Pump Relay K22 | LH front of the engine compartment, in the ECM housing, at position 19 | -- | Cooling System Connector End Views in Engine Cooling
Battery | LH front of engine compartment | -- | --
Body Control Module (BCM) | Mounted on RH A-pillar, behind trim panel | BCM Component Views in Body Control System | BCM Connector End Views in Body Control System
Coolant Fan Test Connector | LH front of the engine compartment, in the ECM housing, at position 5 | -- | Cooling System Connector End Views in Engine Cooling
ECM Cooling Blower | LH front of the engine compartment, attached to the ECM housing | Engine Controls Component Views in Engine Controls | Cooling System Connector End Views in Engine Cooling
ECM Housing | LH front of the engine compartment | Engine Controls Component Views in Engine Controls | --
ECM Relay K48 | LH front of the engine compartment, in the ECM housing, at position 6 | -- | Cooling System Connector End Views in Engine Cooling
Electric Cooling Fan | Front center of the engine compartment, behind the radiator | Cooling System Component Views in Engine Cooling | Cooling System Connector End Views in Engine Cooling
Engine Coolant Fan Resistor | LH side of the engine compartment, mounted beneath the battery | Cooling System Component Views in Engine Cooling | --
Fan Control Relay K26 | LH front of the engine compartment, in the ECM housing, at position 13 | -- | Cooling System Connector End Views in Engine Cooling
Fan Control Relay K28 | LH front of the engine compartment, in the ECM housing, at position 12 | -- | Cooling System Connector End Views in Engine Cooling
Fan Control Relay K52 | LH front of the engine compartment, in the ECM housing, at position 14 | -- | Cooling System Connector End Views in Engine Cooling
Fan Control Relay K67 | LH front of the engine compartment, in the ECM housing, at position 20 | -- | Cooling System Connector End Views in Engine Cooling
Fan Control Relay K87 | LH front of the engine compartment, in the ECM housing, at position 15 | -- | Cooling System Connector End Views in Engine Cooling
Fuse #40 | LH front of the engine compartment, in the ECM housing, at position 23 | -- | --
Fuse #42 | LH front of the engine compartment, in the ECM housing, at position 11 | -- | --
Fuse #50 | LH front of the engine compartment, in the ECM housing, at position 7 | -- | --
Fuse #52 | LH front of the engine compartment, in the ECM housing, at position 24 | -- | --
Fuse Block | Mounted to I/P, lower LH side of the steering column | -- | --
Heater Water Auxiliary Pump | LH front of engine compartment | Cooling System Component Views in Engine Cooling | --
Primary Cooling Fan Temperature Switch | In upper LH side of radiator | Cooling System Component Views in Engine Cooling | --
Secondary Cooling Fan Temperature Switch | In lower LH side of radiator | Cooling System Component Views in Engine Cooling | --
Water Auxiliary Pump | LH front of the engine compartment, to the right of the battery |  | --
C111 | I/P wiring harness to A/C control wiring harness, LH front of the engine compartment | -- | Inline Harness Connector End Views in Wiring Systems
C200B | I/P wiring harness to body wiring harness, at lower LH A-pillar | Power and Grounding Component Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G103 | Body and I/P wiring harnesses, located at the LH front of the engine compartment, near C102, C105 and C106 | Wiper/Washer System Component Views in Wiper/Washer System | --
P104 | In the LH engine compartment, at the front of the ECM housing | -- | --
P110 | Rear LH corner of the engine compartment | -- | --
S108 | A/C control wiring harness, approximately 12 cm from the C111 branch break off | -- | --
S109 | A/C control wiring harness, approximately 12 cm from the C111 branch break off | -- | --
S110 | A/C control wiring harness, approximately 12 cm from the C111 branch break off | -- | --
S111 | A/C control wiring harness, approximately 12 cm from the C111 branch break off | -- | --
S112 | A/C control wiring harness, inside ECM housing, near P104 | -- | --
S113 | A/C control wiring harness, inside ECM housing, near P104 | -- | --
S114 | A/C control wiring harness, inside ECM housing, near P104 | -- | --
S115 | A/C control wiring harness, inside ECM housing, near P104 | -- | --
S116 | A/C control wiring harness, inside ECM housing, near P104 | -- | --
S117 | A/C control wiring harness, inside ECM housing, near P104 | -- | --
S118 | A/C control wiring harness, inside ECM housing, near P104 | -- | --
S125 | A/C control wiring harness, approximately 12 cm from the C111 branch break off | -- | --