For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Evaporator Line Extension Bolt | 20 N·m | 15 lb ft
AIR Injection Crossover Pipe Support Bracket Bolt | 20 N·m | 15 lb ft
Brake Pipe to Master Cylinder | 16 N·m | 12 lb ft
EBTCM/BPMV Heat Shield Screw | 8 N·m | 71 lb in
Lower Steering Gear Heat Shield Nut | 15 N·m | 11 lb ft
Pitman Arm Nut | 160 N·m | 118 lb ft
Power Steering Fluid Flow Control Valve Actuator Screw | 3 N·m | 27 lb in
Power Steering Fluid Reservoir Clamp Bolt | 7 N·m | 62 lb in
Power Steering Gear Inlet Hose to Power Steering Gear | 28 N·m | 21 lb ft
Power Steering Gear Inlet Hose to Power Steering Pump | 28 N·m | 21 lb ft
Power Steering Gear Outlet Hose to Power Steering Gear | 28 N·m | 21 lb ft
Power Steering Pump Bolt | 20 N·m | 15 lb ft
Power Steering Pump Pulley Bolt | 20 N·m | 15 lb ft
Steering Gear Bolt | 40 N·m | 30 lb ft
Steering Column Shaft Coupler Bolt | 22 N·m | 16 lb ft
Steering Gear Coupler Bolt | 22 N·m | 16 lb ft
Upper Steering Gear Heat Shield Bolt | 8 N·m | 71 lb in
Vacuum Booster Nut | 20 N·m | 15 lb ft