For 1990-2009 cars

#### Driver Seat Adjuster Memory Module (Connector C1)

Connector Part Information |

• | ZF 8 -3

• | 8 Way F

• | BLK

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | RED | A5 | B+ from Fuse 35
2 | BLK | F5 | Ground to G103
3 | RED | A40 | B+ from Fuse 35
4 | BRN | X13 | B+ from Fuse 15
5 | BLK | F40 | Ground to G103
6 | BRN/WHT | XM55 | Serial Data
7 | GRY/WHT | RM12 | Door Open Signal
8 | -- | -- | Not Used

#### Driver Seat Adjuster Switch C7 (Connector C7A)

Connector Part Information |

• | 3 Way

• | BLK

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | BLU/PNK | -- | +5 Volt Reference
2 | BLU | -- | Ground
3 | BLU/GRN | -- | Ground

#### Driver Seat Adjuster Switch C7 (Connector C7B)

Connector Part Information |

• | 3 Way

• | BLU

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | BLU/BLK | -- | +5 Volt Reference
2 | BLU/RED | -- | Ground
3 | BLU/YEL | -- | Ground

#### Driver Seat Adjuster Switch C7 (Connector C7C)

Connector Part Information |

• | 3 Way

• | NAT

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | BLU/WHT | -- | +5 Volt Reference
2-3 | -- | -- | Not Used

#### Driver Seat Connector C315

Connector Part Information |

• | ZF 8-6

• | 8 Way F

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | RED/WHT | AM900 | Driver Belt High
2 | BRN/WHT | XM901 | Driver Belt Low
3 | RED | A70 | B+ from Fuse 35
4 | BLK | F66 | Ground to G103
5 | BLK | F39 | Ground to G103
6 | BLK/RED | FA9 | Heated Seat Signal
7 | BLK | F650 | Ground to G103
8 | BRN/BLK | XF21 | Seat Belt Buckled/Unbuckled Signal

#### Driver Seat Heater Relay K55

Connector Part Information |

• | ZF 9-6

• | 9 Way F

• | BLK

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | RED | A240 A241 | B+ from Fuse 20
3 | -- | -- | Not Used
4 | BLK | F240 F241 | Ground to G103
5 | BLK/RED | FA90 | Seat Heater ON Signal
6 | BRN | X321 | B+ from Fuse 15
7 | -- | -- | Not Used
8 | BLK/RED | FA9 FA900 | Seat Heater ON Signal
9 | -- | -- | Not Used

#### Driver Seat Heater Switch

Connector Part Information |

• | ZF 10-7

• | 10 Way F

• | BLK

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | YEL | B901 B902 | Ground
3 | BLK/RED | FA811 | Release Signal, Fuel Door
4 | GRY/YEL | RB31 | Dimmer Signal
5 | BLK | F54 | Ground to G103
6 | BLK/RED | FB700 | Heater ON Signal
7 | BRN | X39 | B+ from Fuse 14
8 | BLK/RED | FA90 | Relay ON Signal
9 | GRY/YEL | RB30 RB31 | Dimmer Signal
10 | BLK | F53 F54 | Ground to G103

#### Driver Seat Recliner Adjuster Actuator Motor C3 (Connector C3A)

Connector Part Information |

• | 2 Way

• | BLK

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | GRY/BRN | -- | Ground for Driver Seat Recliner Actuator Motor
2 | GRY | -- | B+ for Driver Seat Recliner Actuator Motor

#### Driver Seat Recliner Adjuster Actuator Motor C3 (Connector C3B)

Connector Part Information |

• | 3 Way

• | BLK

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | RED | -- | +5 Volt Reference Voltage
2 | YEL | -- | Slider Contact
3 | BLK | -- | Ground

#### Forward/Backward Seat Adjuster Actuator Motor C6 (Connector C6A)

Connector Part Information |

• | 2 Way

• | BLU

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | GRY/BRN | -- | Ground for Driver Seat Recliner Actuator Motor
2 | GRY | -- | B+ for Driver Seat Recliner Actuator Motor

#### Forward/Backward Seat Adjuster Actuator Motor C6 (Connector C6B)

Connector Part Information |

• | 3 Way

• | BLU

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | RED/BLK | -- | +5 Volt Reference Voltage
2 | BLU/YEL | -- | Slider Contact
3 | RED/WHT | -- | Ground

#### Front Height Seat Adjuster Actuator Motor C5 (Connector C5A)

Connector Part Information |

• | 2 Way

• | NAT

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | GRY/BRN | -- | Ground for Driver Seat Recliner Actuator Motor
2 | GRY | -- | B+ for Driver Seat Recliner Actuator Motor

#### Front Height Seat Adjuster Actuator Motor C5 (Connector C5B)

Connector Part Information |

• | 3 Way

• | BLK

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | RED/WHT | -- | +5 Volt Reference
2 | BLU/YEL | -- | Slider Contact
3 | RED/BLK | -- | Ground

#### LH Front Side Door Jamb Switch

Connector Part Information |

• | F 2-42

• | 2 Way F

• | BLK

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | GRY/WHT | RM2 | Door Open Signal
2 | GRY | R2 | Door Open Signal

#### LH Rear Seat Cushion Heater Relay K65

Connector Part Information |

• | ZF 9-6

• | 9 Way F

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | RED | A2 | B+ from Fuse 4
3 | -- | -- | Not Used
4 | BLK | F2 | Ground to G200
5 | BLK/WHT | FM1 | Replay ON Signal
6 | BRN | X2 | B+ from Fuse 15
7 | -- | -- | Not Used
8 | BLK/YEL | FB1 | Heater Element ON Signal
9 | -- | -- | Not Used

#### LH Rear Seat Heater Switch

Connector Part Information |

• | ZF 5-10

• | 5 Way F

• | GRN

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | BLK | F32 F31 | Ground to G200
2 | BLK/WHT | FM300 | Relay ON Signal
3 | BRN | X32 X5 | B+ from Fuse 15
4 | GRY/YEL | RB31 RB30 | Dimmer Signal
5 | BLK/YEL | FB32 | Heater ON Signal

#### Passenger Seat Connector C316

Connector Part Information |

• | ZF 8-6

• | 8 Way F

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | RED/YEL | AB900 | Belt Pretensioner Signal
2 | BRN/YEL | XB901 | Belt Pretensioner Signal
3 | RED | A75 | B+ from Fuse 35
4 | BLK | F67 | Ground to G103
5 | BLK | F38 | Heated Seat Signal
6 | BLK/YEL | FB7 | Heated Seat Signal
7-8 | -- | -- | Not Used

#### Passenger Seat Heater Relay K56

Connector Part Information |

• | ZF 9-6

• | 9 Way F

• | BLK

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | RED | A241 | B+ from Fuse 20
3 | -- | -- | Not Used
4 | BLK | F241 | Ground to G103
5 | BLK/YEL | FB70 | Seat Heater ON Signal
6 | BRN | X321 X320 | B+ from Fuse 15
7 | -- | -- | Not Used
8 | BLK/YEL | FB7 FB700 | Seat Heater ON Signal
9 | -- | -- | Not Used

#### Passenger Seat Heater Switch

Connector Part Information |

• | ZF 10-6

• | 10 Way F

• | BLU

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | YEL | B902 | Fuel Door Release Signal
3 | BLK/RED | FA812 | Rear Compartment Release Relay Signal
4 | GRY/YEL | RB33 | Rear Compartment Release Switch Indicator
5 | BLK | F56 | Ground to G103
6 | BLK/YEL | FB700 | Dimmer Control Signal
7 | BRN | X42 | B+ from Fuse 14
8 | BLK/YEL | FB70 | Heater Relay ON Signal
9 | GRY/YEL | RB33 | Rear Compartment Release Switch Indicator
10 | BLK | F55 F56 | Ground to G103

#### RH Rear Seat Cushion Heater Relay K66

Connector Part Information |

• | ZF 9-6

• | 9 Way F

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | RED | A3 | B+ from Fuse 4
3 | -- | -- | Not Used
4 | BLK | F3 | Ground to G200
5 | BLK/WHT | FM2 | Relay ON Signal
6 | BRN | X3 | B+ from Fuse 15
7 | -- | -- | Not Used
8 | BLK/RED | FA1 | Heater ON Signal
9 | -- | -- | Not Used

#### RH Rear Seat Heater Switch

Connector Part Information |

• | ZF 5-11

• | 5 Way F

• | BLK

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | BLK | F32 | Ground to G200
2 | BLK/WHT | FM11 | Relay ON Signal
3 | BRN | X32 | B+ from Fuse 15
4 | GRY/YEL | RB31 | Dimmer Signal
5 | BLK/RED | FA32 | Heater ON Signal

#### Rear Height Seat Adjuster Actuator C4 (Connector C4A)

Connector Part Information |

• | 2 Way

• | BLK

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | GRY/BRN | -- | Ground for Driver Seat Recliner Actuator Motor
2 | GRY | -- | B+ for Driver Seat Recliner Actuator Motor

#### Rear Height Seat Adjuster Actuator C4 (Connector C4B)

Connector Part Information |

• | 3 Way

• | BLK

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
1 | RED/WHT | -- | +5 Volt Reference
2 | BLU/YEL | -- | Slider Contact
3 | RED/BLK | -- | Ground