For 1990-2009 cars

Table 1: | Cruise Control Release Switch
Table 2: | Cruise Control Switch

#### Cruise Control Release Switch

Connector Part Information |

• | F2-34

• | 2 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN | X110 | Fused Ignition Feed
2 | BLK/BRN | FX888 | Cruise Release Signal

#### Cruise Control Switch

Connector Part Information |

• | ZPF 4-50

• | 4 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/BRN | FX500 | Provides Switch RESUME/DECEL input to ECM
B | BRN | X501 | Fused Ignition Feed
C | BLK/RED | FA300 | Provides ON/OFF Input To ECM
D | BLK/YEL | FB300 | Provides SET/ACCEL Input To ECM