For 1990-2009 cars

### Removal Procedure

1. Remove the headliner. Refer to Headlining Trim Panel Replacement in Interior Trim.
2. Disconnect the front sunroof drain hose from the sunroof drain spigot.
3. Disengage the sunroof drain hose from the attachment points on the windshield pillar.
4. Pull the grommet and a short length of the front drain hose out of the front hinge pillar.
5. Disconnect the grommet from the drain hose.
6. Remove the hose from the vehicle

### Installation Procedure

1. Install the hose to the vehicle
2. Pull the hose out through the hole in the front hinge pillar.
3. Install the grommet onto the end of the hose.
4. Install the grommet into the hole in the front hinge pillar.
5. Connect the hose to the attachments on the windshield pillar.
6. Connect the front sunroof drain hose to the sunroof drain spigot.
7. Install the headliner. Refer to Headlining Trim Panel Replacement in Interior Trim.
8. Inspect sunroof for proper operation.