For 1990-2009 cars

Table 1: | Door Lock Switch
Table 2: | Horn Relay K63
Table 3: | Ignition Switch and Lifting Magnet
Table 4: | Left Front Side Door Jamb Switch
Table 5: | Left Front Side Door Lock Switch
Table 6: | Left Rear Side Door Jamb Switch
Table 7: | Low Beam Relay K131
Table 8: | Park Lamp Relay K130
Table 9: | Right Front Side Door Jamb Switch
Table 10: | Right Front Side Door Lock Switch
Table 11: | Right Rear Side Door Jamb Switch
Table 12: | Theft Deterrent Module (Immobilizer)

#### Door Lock Switch

Connector Part Information |

• | ZFW 3-17

• | 3-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK | F4 | Ground
2 | BRN/PPL | XY810 | Door Open Signal Input
3 | -- | -- | Not Used

#### Horn Relay K63

Connector Part Information |

• | ZF 9-14

• | 9-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | RED | A121 | Fused Battery Feed
3 | -- | -- | Not Used
4 | BRN/WHT | XM30 | Horn ON Signal
5 | -- | -- | Not Used
6 | BRN/WHT | XM1 XM899 | Relay Control
7 | -- | -- | Not Used
8 | BLK | F700 | Ground
9 | -- | -- | Not Used

#### Ignition Switch and Lifting Magnet

Connector Part Information |

• | Ignition Switch ZF6-5

• | 6-Way F

• | Lifting Magnet F2-39

• | 2-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RED | A905 | Fused Battery Feed
2 | GRN | U900 | Ground
U | BRN | X826 | Ignition Positive Voltage Circuit (Terminal 15a)
V | BRN | X1 | Ignition Positive Voltage Circuit (Terminal 15)
X | -- | -- | Not Used
W | RED | A19 | Key-In Ignition Circuit (Terminal W)
Y | RED | A503 | Fused Battery Feed
Z | BLK/RED | FA700 | Starter Enable (Terminal 50)

#### Left Front Side Door Jamb Switch

Connector Part Information |

• | F 2-42

• | 2-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY | RM2 | Door Open Signal
2 | GRY | R2 | Door Open Signal

#### Left Front Side Door Lock Switch

Connector Part Information |

• | F 4-21

• | 4-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/BRN | FX805 | Door Lock Signal
2 | BLK/PPL | FY805 | Door Unlock Signal
3 | RED/BLU | AP807 | Illumination Signal
4 | BLK | F12 | Ground to G200

#### Left Rear Side Door Jamb Switch

Connector Part Information |

• | F 2-42

• | 2-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY | R2 | Door Open Signal
2 | GRY | R1 | Door Open Signal

#### Low Beam Relay K131

Connector Part Information |

• | ZFW 5-20

• | 5-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN/RED | XA810 XA811 | Relay Control
2 | -- | -- | Not Used
3 | AM811 | AM811 | Exterior Lamp Power
4 | YEL | B50 | Lamps ON Signal
5 | RED | A814 | Fused Battery Feed

#### Park Lamp Relay K130

Connector Part Information |

• | ZFW 5-20

• | 5-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN/WHT | XM810 XM815 | Relay Control
2 | -- | -- | Not Used
3 | RED/WHT | AM810 AM811 | Exterior Lamp Power
4 | GRY/GRN | RU812 | Lamps ON Signal
5 | RED | A813 | Fused Battery Feed

#### Right Front Side Door Jamb Switch

Connector Part Information |

• | F 2-42

• | 2-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | GRY | R6 | Door Open Signal

#### Right Front Side Door Lock Switch

Connector Part Information |

• | F 4-21

• | 4-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/BRN | FX805 | Door Lock Signal
2 | BLK/PPL | FY805 | Door Unlock Signal
3 | RED/BLU | AP807 | Illumination Signal
4 | BLK | F12 | Ground to G200

#### Right Rear Side Door Jamb Switch

Connector Part Information |

• | F 2-42

• | 2-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY | R2 | Door Open Signal
2 | GRY | R1 | Door Open Signal

#### Theft Deterrent Module (Immobilizer)

Connector Part Information |

• | F 9-33

• | 9-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BRN/BLU | XP21 | Theft Deterrent Request Signal
3 | -- | -- | Not Used
4 | BLK | F150 | Ground
5 | BRN | X5 | Ignition Positive Voltage
6 | BLU/RED | PA13 | Vehicle Speed Signal
7 | BLU/RED | PA14 | Theft Deterrent Output Signal
8 | BRN/WHT | XM15 | Serial Data (KW 82)
9 | RED | A17 | Battery Positive Voltage