For 1990-2009 cars

Table 1: | Adapter Case
Table 2: | Automatic Transmission Control Indicator
Table 3: | Automatic Transmission Range Switch
Table 4: | Automatic Transmission Winter Mode Switch
Table 5: | Main Case
Table 6: | Vehicle Speed Sensor (VSS) Assembly
Table 7: | Transmission Control Module (TCM)

#### Adapter Case

Connector Part Information |

• | ZPF 4-1

• | 4 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/YEL | FB738 | Torque convertor clutch (TCC) solenoid control signal
B | BLK/PPL | FY740 | Pressure control solenoid (PCS) valve signal HI
C | GRY/RED | RA741 | Pressure control solenoid (PCS) valve signal LO
D | BLU/BLK | PF854 | 12 V TCM power relay signal for torque convertor clutch (TCC) solenoid valve

#### Automatic Transmission Control Indicator

Connector Part Information |

• | ZF 12-3

• | 12 Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BLK | F970 | G103
3-4 | -- | -- | Not Used
5 | BRN | X90 | Fused ignition feed
6 | GRY/GRN | RU500 | Fused battery feed w/ park lamp relay ON
7 | GRY/YEL | RB70 | Dimming control signal
8 | BLK/BLU | FP400 | Trans range switch input A
9 | BLK/GRN | FU400 | Trans range switch input B
10 | BLK/YEL | FB400 | Trans range switch input C
11 | GRY | R400 | Trans range switch input P
12 | -- | -- | Not Used

#### Automatic Transmission Range Switch

Connector Part Information |

• | ZPF 8-3

• | 8 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/BLU | FP733 | Trans range switch output A
B | BLK/GRN | FU726 | Trans range switch output B
C | BLK/YEL | FB708 | Trans range switch output C
D | BRN | X756 | Fused ignition feed
E | BLK/RED | FA501 | P/N switch output to starter solenoid
F | WHT/BLK | MF757 | R signal to rear view mirror
G | GRY | R733 | Trans range switch output P
H | BLK/RED | FA500 | Ignition switch start (position III) signal

#### Automatic Transmission Winter Mode Switch

Connector Part Information |

• | ZPM 4-50

• | 4 Way M

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRN | U102 | Winter mode switch output signal
B | BLK | F960 | G103
C | BRN/GRN | XU100 | 3rd gear indicator control
D | BRN | X14 | Fused ignition feed

#### Main Case

Connector Part Information |

• | 12199508

• | ASM 7F M/P 150 (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLU/YEL | PB743 | 2-3 shift solenoid control
B | GRY/BLK | RF745 | Band apply solenoid control
C | BLU/WHT | PM748 | 1-2 and 3-4 shift solenoid control
D | BLU/BLK | PF954 | 12 V TCM power relay signal for solenoids
E | BRN/GRN | XU716 | TFT sensor return
F | BLK/BLU | FP722 | 5 V reference signal for TFT sensor

#### Vehicle Speed Sensor (VSS) Assembly

Connector Part Information | ZPF 2-2
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BLK/YEL | FB703 | VSS Signal HI
2 | BLU/GRN | PU705 | VSS Signal LO

#### Transmission Control Module (TCM)

Connector Part Information |

• | ZF 88-3

• | 88 Way F Bosch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-3 | -- | -- | Not Used
4 | GRY/BLK | RF745 | Band apply solenoid control
5 | GRY/RED | RA741 | Pressure control solenoid (PCS) LO signal
6 | BLK | F819 | Ground to G103
7 | -- | -- | Not Used
8 | BLK/GRN | FU4 | Trans range switch input B
9 | GRY | R800 | Trans range switch input P
11 | -- | -- | Not Used
12 | BLU | P100 | Sport mode switch input
13 | GRN | U102 | Winter mode switch input
14 | BLU/GRN | PU714 | VSS LO signal
15 | BLK | S40 | VSS shielded ground
16 | -- | -- | Not Used
17 | BLK/YEL | FB800 | Sport mode and transmission malfunction indicator control (2nd design)
18-20 | -- | -- | Not Used
21 | BRN/GRN | XU716 | TFT sensor signal return
22 | BLK/BLU | FP722 | TFT sensor (5V ref) signal
23-24 | -- | -- | Not Used
25 | GRY | R133 | Transmission service indicator control (1st design)
25 | -- | -- | Not Used (2nd design)
26 | RED | A828 | Fused battery feed
27 | BRN/GRN | XU100 | 3rd gear indicator control
28 | BLK | F836 | Ground to G103
29 | -- | -- | Not Used
30 | BLU/WHT | PM748 | 1-2 and 3-4 shift solenoid control
31 | -- | -- | Not Used
32 | BLK/YEL | FB738 | TCC solenoid control
33 | BLU/YEL | PB743 | 2-3 shift solenoid control
34-35 | -- | -- | Not Used
36 | BLK/BLU | FP500 | Trans range switch input A
37 | BLK/YEL | FB709 | Trans range switch input C
38-41 | -- | -- | Not Used
42 | BLK/YEL | FB720 | VSS HI signal
43-48 | -- | -- | Not Used
49 | BRN/GRY | XR888 | CAN interface LO
50 | BRN/PPL | XY888 | CAN interface HI
51 | BRN/WHT | XM12 | Serial data (KW2000)
52 | BLK/PPL | FY740 | Pressure control solenoid (PCS) valve HI signal
53 | BLU/BLK | PF754 | Power relay (12V ref) output
54 | BRN | X837 | Fused ignition feed
55-88 | -- | -- | Not Used