For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Body Control Module (BCM) | Mounted on the lower RH A-pillar, behind the trim panel | Body Control System Component Views in Body Control System | Body Control System Connector End Views in Body Control System
Cellular Telephone | Lower RH A-pillar just below the BCM. | -- | Cellular Communication Connector End Views in Cellular Communication
Data Link Connector (DLC) | Attached to the IP carrier, to the left of the steering column | -- | Data Link Communications Connector End Views in Data Link Communications
Fuse Block | Mounted to the IP, lower LH side of the steering column | -- | --
Inflatable Restraint Sensing and diagnostic and Seat Belt Pretensioner Module | Under the center console, near the parking brake lever | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | SIR Connector End Views in SIR
Radio, AM/FM Stereo and Clock and Tape Player and Compact Disk Player | Center of the IP, below the heater and A/C control | -- | Entertainment Connector End Views in Entertainment
Remote Control Door Lock Receiver | In rear compartment, underneath the LH side of the rear window trim panel. | -- | Keyless Entry Connector End Views in Keyless Entry
Sound Processor Interface | In the rear compartment, in the tray that is attached to the rear deck | -- | Entertainment Connector End Views in Entertainment
C200A | IP wiring harness to body wiring harness, at the lower LH A-pillar | Power and Grounding Component Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C201 | Body wiring harness to cellular phone processing station, located near the RH A pillar near the BCM. | -- | --
C207 (blue connector) | Body wiring harness to IP wiring harness, under the RH front side of the center console | -- | Inline Harness Connector End Views in Wiring Systems
C210 | IP wiring harness to rear amplifier wiring harness, at lower RH A-pillar, next to BCM | Body Control System Component Views in Body Control System | Inline Harness Connector End Views in Wiring Systems
G103 | Body and IP wiring harness, located at the LH front of the engine compartment, underneath the battery tray | Wiper/Washer Component Views in Wiper/Washer System | --
G201 | IP wiring harness, mounted near the relay box | -- | --
S103 | Body wiring harness, approximately 15 cm (6 in) from branch break off for the LH headlamp, towards the EBTCM branch break off | -- | --
S104 | Body wiring harness, approximately 71 cm (28 in) from P103, towards the EBTCM branch break off | -- | --
S203 | Body wiring harness, approximately 3 cm (1.5 in) from the BCM branch Break off | -- | --
S209 | IP wiring harness, approximately 14 cm (6 in) from cruise release switch and stoplamp switch branch break off, to the right of the DLC branch break off | -- | --
S210 | IP wiring harness, near the multifunction relay K134 connector branch break off | -- | --
S232 | IP wiring harness, near the heater and A/C control connector branch break off | -- | --
S241 | IP wiring harness, near the DLC branch breakoff | -- | --
S263 | IP wiring harness, near the multifunction relay K134 connector branch break off | -- | --
S307 | Body wiring harness, base of RH A-pillar, just under conduit | -- | --