For 1990-2009 cars

The SIR Scan Tool Data List contains all the restraint system related parameters that are available on the scan tool. The parameters in the list are arranged in alphabetical order. The column, Data List, indicates the location of the parameter within the scan tool menu selections.

Use the SIR Scan Tool Data List as directed by a diagnostic table or in order to supplement the diagnostic procedures. Begin all of the diagnostic procedures with A Diagnostic System Check - SIR. Use the SIR Scan Tool Data List after the following is determined:

• | There is no published DTC procedure nor published symptom procedure for the customer concern.

• | The DTC or symptom diagnostic procedure indicated by the diagnostic system check does not resolve the customer concern.

The Typical Data Values are obtained from a properly operating vehicle under the conditions specified in the first row of the Scan Tool Data List table. Comparison of the parameter values from the suspect vehicle with the Typical Data Values may reveal the source of the customer concern.

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Ignition ON/Engine OFF/Driver Seat Belt Buckled/Passenger Seat Belt Buckled
Driver Air Bag Res. | Data | Ohms | 2.9 ohms
Ignition | Data | Volts | 12 Volts
Ignition Status | Data | OK/NOK | OK
LH Pretens. Resist. | Data | Ohms | 2.5 ohms
LH Side Air Bag Resist. | Data | Ohms | 2.4 ohms
LH SIS Comm. Error | Data | Error/No Error | No Error
LH SIS Init. Status | Data | OK/NOK | OK
LH SIS Message Status | Data | OK/NOK | OK
Passenger Air Bag Resist. | Data | Ohms | 2.3 ohms
Reset LH Side Air Bag After Deployment | Data | Active/Inactive | Inactive
Reset Pretensioner After Deployment | Data | Active/Inactive | Inactive
Reset RH Side Air Bag After Deployment | Data | Active/Inactive | Inactive
RH Pretens. Resist. | Data | Ohms | 2.4 ohms
RH Side Air Bag Resist. | Data | Ohms | 2.4 ohms
RH SIS Comm. Error | Data | Error/No Error | No Error
RH SIS Init. Status | Data | OK/NOK | OK
RH SIS Message Status | Data | OK/NOK | OK
SDM Configuration | Data | -- | Driv Pass & Side
Warning Lamp | Data | ON/OFF | ON