For 1990-2009 cars

• | Engine Front Crossmember Frame (Longitudinal)

• | Engine Front Crossmember Frame (Diagonal)

• | Frame Diagonal Checking From Right-Center to Left-Rear

• | Frame Diagonal Checking From Left-Center to Right-Rear

• | Rear Axle Cradle Mounting Bolts

• | Diagonal of Engine Compartment Opening

• | Depth (Length) of Engine Compartment

• | Width Between Both Strut Towers

• | Diagonal of Windshield Frame

• | Height of Windshield Frame

• | Diagonal of Front Door Frame

• | Height of Front Door Frame

• | A to B Pillar

• | Diagonal of Rear Door Frame

• | Diagonal of Rear Door Frame

• | Height of Rear Door Frame

• | B to C Pillar

• | Distance Between Both A Pillars (Upper)

• | Distance Between Both B Pillars (Upper)

• | Distance Between Both C Pillars (Upper)

• | Distance Between Both A Pillars (Door Stop)

• | Distance Between Both B Pillars (Door Stop)

• | Distance Between Both C Pillars (at Door Lock)

• | Distance Between Both A Pillars (Lower)

• | Distance Between Both B Pillars (Lower)

• | Distance Between Both C Pillars (Lower)

• | Diagonal of Upper B Pillar to Lower B Pillar

• | Width of Rear Quarter Panel Ends (at Rear Lamp Height)

• | Width of Rear Upper Shock Mounts

• | Depth (Length) of Rear Compartment

• | Diagonal of Rear Compartment Lid Opening

• | Depth (Length) of Rear Compartment Lid Opening

• | Diagonal of Rear Window Frame Opening