For 1990-2009 cars

Table 1: | Accelerator Pedal Position (APP) Sensor
Table 2: | Camshaft Position (CMP) Sensor
Table 3: | Crankshaft Position (CKP) Sensor
Table 4: | Engine Controls Power Relay (K43)
Table 5: | Engine Coolant Temperature (ECT) Sensor
Table 6: | Evaporative (EVAP) Purge Solenoid
Table 7: | Evaporative Vent Valve (EVAP) Solenoid
Table 8: | Fuel Pump and Sender Assembly
Table 9: | Fuel Pump Relay (K44)
Table 10: | Fuel Tank Pressure (FTP) Sensor
Table 11: | Heated Oxygen Sensor (HO2S) - Bank 1, Position 1
Table 12: | Heated Oxygen Sensor (HO2S) - Bank 1, Position 2
Table 13: | Heated Oxygen Sensor (HO2S) - Bank 2, Position 1
Table 14: | Heated Oxygen Sensor (HO2S) - Bank 2, Position 2
Table 15: | Ignition Coil - Bank 1
Table 16: | Ignition Coil - Bank 2
Table 17: | Intake Plenum Switch-Over Solenoid
Table 18: | Intake Resonance Switch-Over Solenoid
Table 19: | Knock Sensor (KS) - Bank 1
Table 20: | Knock Sensor (KS) - Bank 2
Table 21: | Mass Air Flow (MAF) Sensor
Table 22: | Secondary Air Injection Pump
Table 23: | Secondary Air Injection (AIR) Pump Relay K12
Table 24: | Secondary Air Injection (AIR) Solenoid
Table 25: | Sequential Multiport Fuel Injector 1
Table 26: | Sequential Multiport Fuel Injector 2
Table 27: | Sequential Multiport Fuel Injector 3
Table 28: | Sequential Multiport Fuel Injector 4
Table 29: | Sequential Multiport Fuel Injector 5
Table 30: | Sequential Multiport Fuel Injector 6
Table 31: | Throttle Position (TP) Sensor

#### Accelerator Pedal Position (APP) Sensor

Connector Part Information |

• | ZF 9-34

• | 9-Way F (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN/RED | XA40 | Pedal Position 2 Signal Return
2 | BRN/GRY | XR24 | Pedal Position 1 Reference Ground
3 | -- | -- | Not Used
4 | BLK/GRY | FR56 | Pedal Position 1 5V Reference
5 | BRN/BLK | XF8 | Pedal Position 1 Signal Return
6 | BRN/GRN | XU800 | Ground
7 | -- | -- | Not Used
8 | BLK/RED | FA7 | Pedal Position 2 5V Reference
9 | -- | -- | Not Used

#### Camshaft Position (CMP) Sensor

Connector Part Information |

• | ZFW 3-28

• | 3-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN/GRN | XU306 | Sensor Ground
2 | WHT | M381 | CMP Sensor Signal Output
3 | RED/BLU | AP800 | Switched Battery Positive Voltage

#### Crankshaft Position (CKP) Sensor

Connector Part Information |

• | ZFW 3-25

• | 3-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY/BLK | RF78 | CKP Signal High Output
2 | GRY/RED | RA20 | CKP Signal Low Output
3 | BLK | S03 | Shielded Ground

#### Engine Controls Power Relay (K43)

Connector Part Information |

• | ZF 9-31

• | 9-Way (PPL)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | RED | A71 | Fused Battery Feed
3 | -- | -- | Not Used
4 | RED | A73 | Fused Battery Feed
5 | -- | -- | Not Used
6 | BRN/GRY | XR31 | Relay Control
7 | -- | -- | Not Used
8 | RED/BLU | AP75 | Switched B+ From Relay
9 | -- | -- | Not Used

#### Engine Coolant Temperature (ECT) Sensor

Connector Part Information |

• | ZFW 2-83

• | 2-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN/BLU | XP74 | ECT Sensor Signal
2 | BRN/GRN | XU715 | Sensor Ground

#### Evaporative (EVAP) Purge Solenoid

Connector Part Information |

• | ZFW 2-83

• | 2-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RED/BLU | AP108 | B+ From Relay
2 | BRN/RED | XA61 | EVAP Purge Solenoid Valve Control

#### Evaporative Vent Valve (EVAP) Solenoid

Connector Part Information |

• | ZFW 2-83

• | 2 Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED/BLU | AP888 | B+ From Relay
B | BRN/BLK | XF888 | EVAP Tank Solenoid Valve Control

#### Fuel Pump and Sender Assembly

Connector Part Information | ZFW 5-3
--- | ---
Pin | Wire Color | Circuit No. | Function
A | RED/BLU | AP10 | B+ From FUEL PUMP Fuse
B | BLK | F224 | Ground to G103
C | BLK | F30 | Ground to G400
D | BLU/BLK | PF11 | Fuel Level Signal
E | -- | -- | Not Used

#### Fuel Pump Relay (K44)

Connector Part Information |

• | ZF 9-31

• | 9-Way (PPL)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | RED | A72 | Fused Battery Feed
3 | -- | -- | Not Used
4 | RED/BLU | AP76 | B+ From Relay
5 | -- | -- | Not Used
6 | BRN/BLU | XR3 | Relay Control
7 | -- | -- | Not Used
8 | RED/BLU | AP77 | B+ Feed to FUEL PUMP Fuse
9 | -- | -- | Not Used

#### Fuel Tank Pressure (FTP) Sensor

Connector Part Information |

• | ZFW 3-23

• | 3-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLU/BLK | PF1 | 5V Reference
2 | BRN/GRN | XU1 | Sensor Ground
3 | BRN/YEL | XB1 | Fuel Pressure Sensor Signal

#### Heated Oxygen Sensor (HO2S) - Bank 1, Position 1

Connector Part Information | ZFW 6-15
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BRN/RED | XA43 | Lambda Sensor Pump Current Input
2 | BRN/BLU | XP19 | HO2S Signal
3 | BRN/WHT | XM30 | HO2S Reference Ground
4 | BRN/GRY | XR11 | HO2S Heater Control
5 | RED/BLU | AP122 | Fused Battery Feed
6 | BRN/GRN | XU462 | Lambda Sensor Pump Current Output

#### Heated Oxygen Sensor (HO2S) - Bank 1, Position 2

Connector Part Information | ZMW 4-2
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP951 | Fused Battery Feed
2 | BRN/WHT | XM951 | HO2S Heater Control
3 | BRN/GRN | XU950 | HO2S Reference Ground
4 | BRN/BLU | XP961 | HO2S Signal

#### Heated Oxygen Sensor (HO2S) - Bank 2, Position 1

Connector Part Information | ZFW 6-15
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BRN/RED | XA610 | Lambda Sensor Pump Current Input
2 | BRN/BLU | XP18 | HO2S Signal
3 | BRN/WHT | XM309 | HO2S Reference Ground
4 | BRN/GRY | XR61 | HO2S Heater Control
5 | RED/BLU | AP124 | Fused Battery Feed
6 | BRN/GRN | XU464 | Lambda Sensor Pump Current Output

#### Heated Oxygen Sensor (HO2S) - Bank 2, Position 2

Connector Part Information | ZMW 4-2
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP950 | Fused Battery Feed
2 | BRN/WHT | XM950 | HO2S Heater Control
3 | BRN/GRN | XU960 | HO2S Reference Ground
4 | BRN/BLU | XP960 | HO2S Signal

#### Ignition Coil - Bank 1

Connector Part Information |

• | ZFW 6-7

• | 6 Way F BOSCH (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK | F50 | Ground
2 | BRN | X68 | Switched Ignition Feed
3 | GRY/BLK | RF50 | Cyl. 5 Ignition Control
4 | BLK/YEL | FB60 | Cyl. 3 Ignition Control
5 | BLK/RED | FA70 | Cyl. 1 Ignition Control
6 | -- | -- | Not Used

#### Ignition Coil - Bank 2

Connector Part Information |

• | ZFW 6-11

• | 6 Way F BOSCH (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK | F60 | Ground
2 | BRN | X69 | Switched Ignition Feed
3 | GRY/BLK | RF51 | Cyl. 6 Ignition Control
4 | BLK/YEL | FB61 | Cyl. 4 Ignition control
5 | BLK/RED | FA71 | Cyl. 2 Ignition Control
6 | -- | -- | Not Used

#### Intake Plenum Switch-Over Solenoid

Connector Part Information | ZFW 2-40
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BRN/GRN | XU35 | Intake Plenum Switch-Over Solenoid Valve Control
2 | RED/BLU | AP105 | B+ From Relay

#### Intake Resonance Switch-Over Solenoid

Connector Part Information | ZFW 2-40
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BRN/GRN | XU7 | Intake Resonance Switch-Over Solenoid Valve Control
2 | RED/BLU | AP104 | B+ From Relay

#### Knock Sensor (KS) - Bank 1

Connector Part Information | ZFW 2-107
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BRN/WHT | XM70 | KS Bank 1 Signal
2 | BRN/GRN | XU420 | KS Reference Ground

#### Knock Sensor (KS) - Bank 2

Connector Part Information | ZFW 2-89
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BRN/WHT | XM40 | KS Bank 2 Signal
2 | BRN/GRN | XU410 | KS Reference Ground

#### Mass Air Flow (MAF) Sensor

Connector Part Information |

• | ZFW 5-7

• | 5 Way F BOSCH (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN/BLK | XF30 | IAT Sensor Signal
2 | RED/BLU | AP84 | B+ From Relay
3 | BRN/GRN | XU304 | Sensor Ground
4 | BLU/BLK | PF107 | 5 V Reference
5 | GRY/RED | RA40 | MAF Sensor Signal

#### Secondary Air Injection Pump

Connector Part Information | ZFW 2-24
--- | ---
Pin | Wire Color | Circuit No. | Function
A | PPL | Y110 | Pump Control
B | BLK | F110 | Ground to G104

#### Secondary Air Injection (AIR) Pump Relay K12

Connector Part Information |

• | ZF 9-32

• | 9-Way (BRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | PPL | Y110 | Pump ON Signal
3 | -- | -- | Not Used
4 | RED/BLU | AP200 | B+ From Relay
5 | BLK | F200 | Ground to G103
6 | BRN/GRY | XR200 | Relay Control
7 | -- | -- | Not Used
8 | RED | A730 | Fused Battery Feed
9 | -- | -- | Not Used

#### Secondary Air Injection (AIR) Solenoid

Connector Part Information | ZFW 2-35
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP952 | B+ From Relay
2 | BRN/YEL | XB952 | Solenoid Valve Control

#### Sequential Multiport Fuel Injector 1

Connector Part Information | ZFW 2-44
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP61 | B+ From Relay
2 | BRN/YEL | XB17 | Fuel Injector #1 Control

#### Sequential Multiport Fuel Injector 2

Connector Part Information | ZFW 2-44
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP63 | B+ From Relay
2 | BRN/GRN | XU16 | Fuel Injector #2 Control

#### Sequential Multiport Fuel Injector 3

Connector Part Information | ZFW 2-44
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP64 | B+ From Relay
2 | BRN/BLU | XP35 | Fuel Injector #3 Control

#### Sequential Multiport Fuel Injector 4

Connector Part Information | ZFW 2-44
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP62 | B+ From Relay
2 | BRN/RED | XA34 | Fuel Injector #4 Control

#### Sequential Multiport Fuel Injector 5

Connector Part Information | ZFW 2-44
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP65 | B+ From Relay
2 | BRN/BLK | XF15 | Fuel Injector #5 Control

#### Sequential Multiport Fuel Injector 6

Connector Part Information | ZFW 2-44
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP66 | B+ From Relay
2 | BRN/PPL | XY33 | Fuel Injector #6 Control

#### Throttle Position (TP) Sensor

Connector Part Information |

• | ZFW 6-10

• | 6 Way F AMP (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/WHT | FM10 | Throttle Valve Motor Ground
2 | BRN/GRN | XU30 | Sensor Ground
3 | BLU/BLK | PF102 | 5 V Reference
4 | BRN/YEL | XB10 | Throttle Valve Motor Power
5 | BRN/BLU | XP53 | TP Sensor 2 Signal
6 | WHT | M24 | TP Sensor 1 Signal