For 1990-2009 cars

Application | Metric | English
Compressor Replacement - Add ___ of PAG refrigerant oil. | 60 ml* | 2 oz*
Receiver/Dehydrator Replacement - Add ___ more PAG refrigerant oil. | 30 ml* | 1 oz*
Evaporator Replacement - Add ___ of PAG refrigerant oil. | 90 ml* | 3 oz*
Condenser Replacement - Add ___ of PAG refrigerant oil. | 30 ml* | 1 oz*
* If more than the specified amount of PAG oil was drained, add the equal amount drained.