For 1990-2009 cars

### Programming The Memory Seat Positions

You can program the driver seat adjuster memory module for three memory positions. You can program the driver seat, the LH and RH outside rear view mirrors and the inside rear view mirror to the three different positions. The following instructions are for programming the memory seat positions:

1. Turn the ignition switch to the ON position.
2. Adjust the driver's seat to a comfortable position.
3. Adjust the inside and outside rear view mirrors to a comfortable position.
4. Press the memory button and the number 1 button at the same time. This stores the position of the driver seat, the inside rear view mirror and the outside rear view mirrors in the driver seat adjuster memory module.
5. You can program the driver seat and mirrors for 2 additional drivers by repeating the above steps and pressing the number 2 or 3 instead of number 1.