For 1990-2009 cars

Table 1: | Door Lock Switch
Table 2: | Horn Relay K63
Table 3: | Ignition Switch and Lifting Magnet
Table 4: | LH Front Side Door Jamb Switch
Table 5: | LH Front Side Door Lock Switch
Table 6: | LH Rear Side Door Jamb Switch
Table 7: | Low Beam Relay K131
Table 8: | Park Lamp Relay K130
Table 9: | Remote Control Door Lock Receiver (RCDLR)
Table 10: | RH Front Side Door Jamb Switch
Table 11: | RH Front Side Door Lock Switch
Table 12: | RH Rear Side Door Jamb Switch
Table 13: | Theft Deterrent Module Connector

#### Door Lock Switch

Connector Part Information | 0688030101
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BLK | F4 | Ground to G200
2 | BRN/PPL | XY810 | Door open signal input

#### Horn Relay K63

Connector Part Information | ZF 9-14
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | -- | -- | Not used
2 | RED | A121 | B+ from Fuse #8
3 | -- | -- | Not used
4 | BRN/WHT | XM30 | Horn ON Signal
5 | -- | -- | Not used
6 | BRN/WHT | XM1 XM899 | Switch Signal
7 | -- | -- | Not used
8 | BLK | F700 | Ground to G103
9 | -- | -- | Not used

#### Ignition Switch and Lifting Magnet

Connector Part Information | ZF6-5
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | GRN | A905 | B+ from fuse #24
2 | GRN | U900 | Brake to shift signal
U | BRN | X826 | B+ in the ON position
V | BRN | X1 | B+ in the ON or START position
W | RED | A19 | B+ when the key is inserted
Y | RED | A503 | B+ form fuse V2
Z | BLK/RED | FA700 | Starter solenoid signal

#### LH Front Side Door Jamb Switch

Connector Part Information | F 2-42
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | GRY | RM2 | Door Open Signal
2 | GRY | R2 | Door Open Signal

#### LH Front Side Door Lock Switch

Connector Part Information | F 4-21
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BLK/BRN | FX805 | Door Lock Signal
2 | BLK/PPL | FY805 | Door Unlock Signal
3 | RED/BLU | AP807 | Illumination Signal
4 | BLK | F12 | Ground to G200

#### LH Rear Side Door Jamb Switch

Connector Part Information | F 2-42
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | GRY | R2 | Door Open Signal
2 | GRY | R1 | Door Open Signal

#### Low Beam Relay K131

Connector Part Information | ZFW 5-20
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BRN/RED | XA810 XA811 | Relay Control
2 | -- | -- | Not used
3 | AM811 | AM811 | Exterior Lamp Power
4 | YEL | B50 | Lamps ON Signal
5 | RED | A814 | B+ from Fuse V3

#### Park Lamp Relay K130

Connector Part Information | ZFW 5-20
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BRN/WHT | XM810 XM815 | Relay Control
2 | -- | -- | Not used
3 | RED/WHT | AM810 AM811 | Exterior Lamp Power
4 | GRY/GRN | RU812 | Lamp ON Signal
5 | RED | A813 | B+ from Fuse V3

#### Remote Control Door Lock Receiver (RCDLR)

Connector Part Information |

• | 12045813

• | ASM 4F M/P 150 (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | A823 | B+ from fuse #28
B | BRN/WHT | XM832 | Class 2 serial data
C | BLK/RED | F802 | Ground to G103
D | -- | -- | Not Used

#### RH Front Side Door Jamb Switch

Connector Part Information | F 2-42
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | -- | -- | Not used
2 | GRY | R6 | Door Open Signal

#### RH Front Side Door Lock Switch

Connector Part Information | F 4-21
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BLK/BRN | FX805 | Door Lock Signal
2 | BLK/PPL | FY805 | Door Unlock Signal
3 | RED/BLU | AP807 | Illumination Signal
4 | BLK | F12 | Ground to G200

#### RH Rear Side Door Jamb Switch

Connector Part Information | F 2-42
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | GRY | R2 | Door Open Signal
2 | GRY | R1 | Door Open Signal

#### Theft Deterrent Module Connector

Connector Part Information | F 9-33
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | -- | -- | Not Used
2 | BRN/BLU | XP21 | Theft deterrent request signal
3 | -- | -- | Not Used
4 | BLK | F150 | Ground
5 | BRN | X5 | Ignition switch input signal
6 | BLU/RED | PA13 | Vehicle speed signal
7 | BLU/RED | PA14 | Theft deterrent output signal
8 | BRN/WHT | XM15 | Serial data
9 | RED | A17 | Battery input