For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Automatic Transmission Shift Lock Control Solenoid | Attached to the automatic transmission control base, to the left of the shift lever | -- | --
Automatic Transmission Shift Lock Control Switch | Attached to the automatic transmission control base, to the right of the shift lever | -- | --
Automatic Transmission Shift Lock/Unlock Switch | Attached to the automatic transmission control base, to the left of the shift lever | -- | --
Body Control Module (BCM) | Mounted on the lower RH A-pillar, behind the trim panel | Body Control System Component Views in Body Control System | Body Control System Connector End Views in Body Control System
Door Lock Relay K135 | Mounted on the lower RH A-pillar, behind the BCM | Body Control System Component Views in Body Control System | Body Control System Connector End Views in Body Control System
Driver Seat Adjuster Memory Module | Attached to the underside of the driver's seat | Power Seat Component Views in Seats | Power Seat Connector End Views in Seats
Front Side Door Jamb Switch (LH) | Lower LH A-pillar | -- | Lighting Systems Connector End Views in Lighting Systems
Front Side Door Jamb Switch (RH) | Lower RH A-pillar | -- | Lighting Systems Connector End Views in Lighting Systems
Front Side Door Lock Actuator (LH) | Mounted inside of the LH front side door | Power Door Systems Component Views | Power Door Systems Connector End Views
Front Side Door Lock Actuator (RH) | Mounted inside of the RH front side door | Power Door Systems Component Views | Power Door Systems Connector End Views
Front Side Door Lock Switch (LH) | Mounted to the inside LH front side door trim panel | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | Lighting Systems Connector End Views in Lighting Systems
Front Side Door Lock Switch (RH) | Mounted to the inside RH front side door trim panel | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | Lighting Systems Connector End Views in Lighting Systems
Front Side Door Window Regulator Motor (LH) | Mounted inside of the LH front side door | Power Door Systems Component Views | Power Door Systems Connector End Views
Front Side Door Window Regulator Motor (RH) | Mounted inside of the RH front side door | Power Door Systems Component Views | Power Door Systems Connector End Views
Front Side Door Window Switch (LH) | Center console | -- | Power Door Systems Connector End Views
Front Side Door Window Switch (RH) | Center console | -- | Power Door Systems Connector End Views
Fuel Tank Filler Door Lock Release Switch | Center of the IP, to the left of the heater and A/C control | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | Body Rear End Connector End Views in Body Rear End
Fuse Block | Mounted to the IP, lower LH side of the steering column | -- | --
Headlamp Switch | LH side of the IP | -- | Lighting Systems Connector End Views in Lighting Systems
Heated Outside Rear View Mirror and Rear Window Defogger Relay K35 | Lower IP, to the RH side of the steering column, on the relay box (Roman numeral III) | -- | Stationary Windows Connector End Views in Stationary Windows
Outside Rear View Mirror (LH) | Attached to the LH front side door | Power Door Systems Component Views | Power Door Systems Connector End Views
Outside Rear View Mirror (RH) | Attached to the RH front side door | Power Door Systems Component Views | Power Door Systems Connector End Views
Outside Remote Control Rear View Mirror Switch | Mounted to the inside LH front side door trim panel | Power Door Systems Component Views | Power Door Systems Connector End Views
Rear Side Door Lock Actuator (LH) | Mounted inside of the LH rear side door | Power Door Systems Component Views | Power Door Systems Connector End Views
Rear Side Door Lock Actuator (RH) | Mounted inside of the RH rear side door | Power Door Systems Component Views | Power Door Systems Connector End Views
Rear Side Door Window Regulator Motor (LH) | Mounted inside of the LH rear side door | Power Door Systems Component Views | Power Door Systems Connector End Views
Rear Side Door Window Regulator Motor (RH) | Mounted inside of the RH rear side door | Power Door Systems Component Views | Power Door Systems Connector End Views
Rear Side Door Window Switch (LH) | Mounted on the LH rear side door trim panel | Power Door Systems Component Views | Power Door Systems Connector End Views
Rear Side Door Window Switch (RH) | Mounted on the RH rear side door trim panel | Power Door Systems Component Views | Power Door Systems Connector End Views
Rear Window Lockout Switch | Located next to the LH front side door window switch, in the center console | -- | --
Stop Lamp Switch | Attached to the brake pedal | -- | Lighting Systems Connector End Views in Lighting Systems
C200A | IP wiring harness to body wiring harness, at lower LH A-pillar | Power and Grounding Component Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200B | IP wiring harness to body wiring harness, at lower LH A-pillar | Power and Grounding Component Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C205 | IP wiring harness to automatic transmission control switches, attached to the automatic transmission control base, to the right of the shift lever | -- | Inline Harness Connector End Views in Wiring Systems
C303 | Body wiring harness to LH rear side door wiring harness, inside the lower LH B-pillar | Power Door Systems Component Views | Inline Harness Connector End Views in Wiring Systems
C304 | Body wiring harness to RH rear side door wiring harness, inside the lower RH B-pillar | Power Door Systems Component Views | Inline Harness Connector End Views in Wiring Systems
C310 | Body wiring harness to the driver seat adjuster memory module, underneath the LH side of the driver's seat | -- | Inline Harness Connector End Views in Wiring Systems
C500 | Body wiring harness to the LH front side door wiring harness, at lower LH A-pillar, near G200 | Power Door Systems Component Views | Inline Harness Connector End Views in Wiring Systems
C600 | Body wiring harness to the RH front side door wiring harness, at lower RH A-pillar | Power Door Systems Component Views | Inline Harness Connector End Views in Wiring Systems
G103 | Body and IP wiring harness, located at the LH front of the engine compartment, underneath the battery tray | Wiper/Washer Component Views in Wipers/Washer Systems | --
P103 | Lower LH A-pillar, forward of G200 | Power and Grounding Component Views in Wiring Systems | --
P110 | Rear LH corner of the engine compartment | -- | --
P300 | At the lower RH B-pillar | -- | --
P301 | At the lower LH B-pillar | -- | --
P500 | In the LH front side door, approximately 12 cm (5 in) from the outside remote control rear view mirror switch connector branch break off | -- | --
P600 | In the RH front side door, approximately 25 cm (10 in) from the RH front side door lock switch connector branch break off | -- | --
P700 | Between the front of the LH rear side door and the lower LH B-pillar | Power Door Systems Component Views | --
P701 | In the LH rear side door, approximately 20 cm (8 in) from the LH rear side door courtesy lamp connector branch break off | -- | --
P800 | Between the front of the RH rear side door and the lower RH B-pillar | Power Door Systems Component Views | --
P801 | In the RH rear side door, approximately 20 cm (8 in) from the RH rear side door courtesy | -- | --
S103 | Body wiring harness, approximately 27 cm (10 in) from P107 | -- | --
S133 | Body wiring harness, approximately 120 cm (48 in) from the C200 branch break off | -- | --
S134 | Body wiring harness, approximately 120 cm (48 in) from the C200 branch break off | -- | --
S135 | Body wiring harness, approximately 120 cm (48 in) from the C200 branch break off | -- | --
S140 | IP wiring harness, near the brake fluid minimum capacity sensor connector branch break off | -- | --
S200 | IP wiring harness, near the DLC branch break off | -- | --
S217 | IP wiring harness, near the multifunction relay K134 connector branch break off | -- | --
S233 | Body wiring harness, in center console at the front side door window switch RH | -- | --
S234 | Body wiring harness, in center console at the front side door window switch RH | -- | --
S250 | IP wiring harness, near the gauge cluster connector branch break off | -- | --
S251 | IP wiring harness, near the G201 branch break off | -- | --
S252 | IP wiring harness, near the G201 branch break off | -- | --
S264 | Body wiring harness, near the G200 branch break off | -- | --
S270 | Body wiring harness, approximately 62 cm (25 in) from the C200 branch break off, toward the driver's side | -- | --
S271 | Body wiring harness, approximately 62 cm (25 in) from the C200 branch break off, toward the driver's side | -- | --
S272 | Body wiring harness, approximately 62 cm (25 in) from the C200 branch break off, toward the driver's side | -- | --
S273 | Body wiring harness, approximately 62 cm (25 in) from the C200 branch break off, toward the driver's side | -- | --
S277 | IP wiring harness, Attached to buss-bar on the automatic transmission shift lever base | -- | --
S304 | Body wiring harness, approximately 23 cm (8 in) from the RCDLR branch break off | -- | --
S305 | Body wiring harness, console wiring branch, approximately 5 cm (2 in) from the break off | -- | --
S306 | Body wiring harness, console wiring branch, approximately 5 cm (2 in) from the break off | -- | --
S307 | Body wiring harness, base of RH A-pillar, just under conduit | -- | --
S308 | Body wiring harness, base of RH A-pillar, just under conduit | -- | --
S309 | Body wiring harness, base of RH A-pillar, just under conduit | -- | --
S311 | Body wiring harness, approximately 23 cm (8 in) from the RCDLR branch break off | -- | --
S312 | Body wiring harness, base of LH A-pillar, just under conduit | -- | --
S313 | Body wiring harness, base of LH A-pillar, just under conduit | -- | --
S314 | Body wiring harness, approximately 23 cm (8 in) from the RCDLR branch break off | -- | --
S500 | LH front side door wiring harness, approximately 31 cm (13 in) from the outside rear view mirror connector branch break off | -- | --
S502 | LH front side door wiring harness, approximately 26 cm (10 in) from the C500 branch break off | -- | --
S504 | LH front side door wiring harness, approximately 26 cm (10 in) from the C500 branch break off | -- | --
S505 | LH front side door wiring harness, approximately 31 cm (13 in) from the outside rear view mirror connector branch break off | -- | --
S600 | RH front side door wiring harness, approximately 26 cm (10 in) from the C600 branch break off | -- | --
S602 | RH front side door wiring harness, approximately 26 cm (10 in) from the C600 branch break off | -- | --
S700 | LH rear side door wiring harness, approximately 28 cm (12 in) from P700 | -- | --
S800 | RH rear side door wiring harness, approximately 28 cm (12 in) from P800 | -- | --