For 1990-2009 cars

### Removal Procedure

1. Remove the rear seatback center armrest. Refer to Rear Seat Armrest Replacement .
2. Remove the cover and the foam from the rear seatback center armrest by unzipping and pulling off.

### Installation Procedure

1. Install the cover and the foam to the rear seatback center armrest by pulling over the pad and zipping close.
2. Install the rear seatback center armrest. Refer to Rear Seat Armrest Replacement .