For 1990-2009 cars

#### Fastener Tightening Specifications Table

Application | Specification
--- | ---
Metric | English
Catalytic Converter Support Bracket to Converter Bolt | 20 N·m | 15 lb ft
Console Rear Support Nut | 4 N·m | 35 lb in
Drive Flange Nut | 100 N·m | 74 lb ft
Exhaust Muffler to Catalytic Converter Bolt | 40 N·m | 30 lb ft
Exhaust Muffler to Catalytic Converter Nut | 40 N·m | 30 lb ft
Flywheel to Torque Converter Bolts | 30 N·m | 22 lb ft
Force Motor Solenoid Valve Bolt | 10 N·m | 87 lb in
Front Oil Pan Bolt | 11 N·m | 96 lb in
Oil Cooler Inlet Pipe Fitting at Transmission | 25 N·m | 18 lb ft
Oil Cooler Outlet Pipe Fitting at Transmission | 30 N·m | 22 lb ft
Oil Cooler Pipe Fitting (Lower at Radiator) | 25 N·m | 18 lb ft
Oil Cooler Pipe Fitting (Upper at Radiator) | 25 N·m | 18 lb ft
Oil Pan Bolt | 11 N·m | 96 lb in
Oil Pan Fill Plug | 45 N·m | 33 lb ft
Oil Pressure Test Hole Plug | 12 N·m | 106 lb in
Propeller Shaft Coupling Bolt | 95 N·m | 70 lb ft
Rear Air Duct Front Support Nut | 8 N·m | 71 lb in
Shift Lever Rod Adjustment Bolt | 8 N·m | 71 lb in
Torque Converter Clutch Solenoid Valve Bolt | 10 N·m | 87 lb in
Transmission Case Extension Bolt | 32 N·m | 23 lb ft
Transmission Control Selector Switch Bolt | 13 N·m | 115 lb in
Transmission Crossmember to Body Bolt | 45 N·m | 33 lb ft
Transmission Crossmember to Mount Nut | 20 N·m | 15 lb ft
Transmission Housing to Engine Block Bolt | 60 N·m | 44 lb ft
Transmission Housing to Engine Oil Pan Bolt | 20 N·m | 15 lb ft
Transmission Mount Bolt | 40 N·m | 30 lb ft
Transmission Oil Filter Bolt | 20 N·m | 15 lb ft
Transmission Speed Sensor Bolt | 9 N·m | 78 lb in

#### Fastener Tightening Specifications

Description of Usage | Reference Number | Quantity | Size | Specification
--- | --- | --- | --- | ---
Center Support to Adapter Case Bolt | 31 | 8 | 5/16x18UNC-2Ax22 | 25 N·m (18 lb ft)
Control Valve Assembly to Adapter Case | 109 | 7 | 5/16x18UNC-2Ax2" | 20 N·m (15 lb ft)
Control Valve Assembly to Main Case | 70 | 7 | 5/16x18UNC-2Ax2" | 20 NM (15 lb ft)
Converter Housing to Case Bolt | 4 | 7 | M10x1.5x172 | 40 N·m (29 lb ft)
Converter Housing to Oil Pump Bolt | 5 | 5 | 5/16x18UNC-2Ax28.5 | 20 NM (15 lb ft)
Converter Housing Oil Seal Bolt (Torx®) | 2 | 3 | M4x0.7x10 | 3 NM (26 lb in)
Detent Roller and Spring Bolt | 70 | 2 | 5/16"x18UNC-2Ax2" | 20 N·m (15 lb ft)
Drive Flange | 47 | 1 | M22x1.5x18 | 105 N·m (74 ft lb)
Forward Band Servo Cover | 90 | 4 | 1/4"x20UNC-2Ax1.5" | 25 N·m (18 lb ft)
Main Case Space Plate Bolt | 89 | 2 | 1/4x20UNC-2Ax9/16" | 13 N·m (113 lb in)
Oil Cooler Inlet Pipe Fitting (At TRS) | 35 | 1 | M16x1.5x10 | 30 N·m (23 lb ft)
Oil Cooler Outlet Pipe Fitting (At TRS) | 34 | 1 | M16x1.5x10 | 30 N·m (23 lb ft)
Oil Pan to Adapter Case | 23 | 12 | M6x1.0x18 | 11 N·m (96 lb in)
Oil Pan to Main Case | 23 | 16 | M6x1.0x18 | 11 N·m (96 lb in)
Oil Pan Overfill Plug | 108 | 1 | M14x1.5x12 | 45 N·m (34 lb ft)
Oil Pressure Test Hole Plug | 7 | 1 | 1/8NPTFx27x11.65 | 12 N·m (104 lb in)
Pressure Control Solenoid Valve | 402 | 1 | 1/4x20UNC-2Ax9/16" | 10 N·m (87 lb in)
Torque Convertor Clutch Solenoid Valve Bolt | 402 | 1 | 1/4"x20UNC-2Ax9/16" | 13 N·m (87 lb in)
Transmission Case Extension Bolt | 52 | 7 | 3/8x16UNC-2Ax1.5" | 32 N·m (24 lb ft)
Transmission Oil Filter Bolt | 70 | 3 | 5/16"x18UNC-2Ax2" | 20 N·m (15 lb ft)
Transmission Speed Sensor | 46 | 1 | M6x1.0x20 | 9 N·m (78 lb in)