For 1990-2009 cars

#### Fastener Tightening Specifications

Application | Specification
--- | ---
Metric | English
Adapter Case Control Valve Assembly | 20 N·m | 15 lb ft
Center Support To Adapter Case Bolt | 25 N·m | 18 lb ft
Converter Housing To Case Bolt | 40 N·m | 29 lb ft
Converter Housing to Oil Pump Bolt | 20 N·m | 15 lb ft
Converter Housing Oil Seal Bolt | 3 N·m | 26 lb in
Drive Flange | 105 N·m | 74 lb ft
Flex Plate To Torque Converter Bolt | 45 N·m | 34 lb ft
Main Case Control Valve Assembly | 20 N·m | 15 lb ft
Main Case Space Plate Bolt | 13 N·m | 113 lb in
Oil Cooler Inlet Pipe Fitting (At TRS) | 25 N·m | 19 lb ft
Oil Cooler Outlet Pipe Fitting (At TRS) | 30 N·m | 23 lb ft
Oil Pan Bolt-Adapter Case | 11 N·m | 96 lb in
Oil Pan Bolt-Main Case | 11 N·m | 96 lb in
Oil Pan Overfill Plug | 45 N·m | 34 lb ft
Oil Pressure Test Hole Plug | 12 N·m | 104 lb in
Pressure Control Solenoid Valve | 10 N·m | 87 lb in
Third Clutch Servo Cover Bolt | 25 N·m | 18 lb ft
Torque Converter Clutch Solenoid Valve Bolt | 10 N·m | 87 lb in
Transmission Case Extension Bolt | 32 N·m | 24 lb ft
Transmission Oil Filter Bolt | 20 N·m | 15 lb ft
Transmission Speed Sensor | 9 N·m | 78 lb in

#### Fastener Tightening Specifications Table

Application | Specification
--- | ---
Metric | English
Catalytic Converter Support Bracket to Converter Bolt | 20 N·m | 15 lb ft
Console Rear Support Nut | 4 N·m | 35 lb in
Drive Flange Nut | 100 N·m | 74 lb ft
Exhaust Muffler to Catalytic Converter Bolt | 40 N·m | 30 lb ft
Exhaust Muffler to Catalytic Converter Nut | 40 N·m | 30 lb ft
Flywheel to Torque Converter Bolts | 30 N·m | 22 lb ft
Force Motor Solenoid Valve Bolt | 10 N·m | 87 lb in
Front Oil Pan Bolt | 11 N·m | 96 lb in
Oil Cooler Inlet Pipe Fitting at Transmission | 25 N·m | 18 lb ft
Oil Cooler Outlet Pipe Fitting at Transmission | 30 N·m | 22 lb ft
Oil Cooler Pipe Fitting (Lower at Radiator) | 25 N·m | 18 lb ft
Oil Cooler Pipe Fitting (Upper at Radiator) | 25 N·m | 18 lb ft
Oil Pan Bolt | 11 N·m | 96 lb in
Oil Pan Fill Plug | 45 N·m | 33 lb ft
Oil Pressure Test Hole Plug | 12 N·m | 106 lb in
Propeller Shaft Coupling Bolt | 95 N·m | 70 lb ft
Rear Air Duct Front Support Nut | 8 N·m | 71 lb in
Shift Lever Rod Adjustment Bolt | 8 N·m | 71 lb in
Torque Converter Clutch Solenoid Valve Bolt | 10 N·m | 87 lb in
Transmission Control Selector Switch Bolt | 13 N·m | 115 lb in
Transmission Crossmember to Body Bolt | 45 N·m | 33 lb ft
Transmission Crossmember to Mount Nut | 20 N·m | 15 lb ft
Transmission Case Extension Bolt | 32 N·m | 23 lb ft
Transmission Housing to Engine Oil Pan Bolt | 20 N·m | 15 lb ft
Transmission Housing to Engine Block Bolt | 60 N·m | 44 lb ft
Transmission Mount Bolt | 40 N·m | 30 lb ft
Transmission Oil Filter Bolt | 20 N·m | 15 lb ft
Transmission Speed Sensor Bolt | 9 N·m | 78 lb in