For 1990-2009 cars

#### Fuel Tank Filler Door Lock Release Switch

Connector Part Information | ZF 10-7
--- | ---
Pin | Wire Color | CKT No. | Function
1 | -- | -- | Not used
2 | YEL | B901 B902 | Ground
3 | BLK/RED | FA811 | Release signal, fuel door
4 | GRY/YEL | RB31 RB32 | Dimmer signal
5 | BLK | F54 F55 | Ground to G103
6 | BLK/YEL | FB700 | Heater ON signal
7 | BRN | X39 X42 | B+ from fuse 14
8 | BLK/RED | FA90 | Relay ON signal
9 | GRY/YEL | RB30 RB31 | Dimmer signal
10 | BLK | F53 F54 | Ground to G103

#### Ignition Switch and Lifting Magnet

Connector Part Information | ZF 6-5
--- | ---
Pin | Wire Color | CKT No. | Function
1 | RED | A905 | B+ from fuse 24
2 | GRN | U900 | Brake to shift signal
U | BRN | X826 | B+ in the ON position
V | BRN | X1 | B+ in the BULB TEST position
W | RED | A19 | B+ when the key is inserted
Y | RED | A503 | B+ form fuse V2
Z | BLK/RED | FA700 | Starter solenoid signal

#### Stop Lamp Switch

Connector Part Information | ZF 4-6
--- | ---
Pin | Wire Color | CKT No. | Function
1 | RED | A401 | B+ from fuse 12
2 | BLK/YEL | FB101 | Brake lamp ON signal
3 | BRN | X11 | B+ from fuse 2
4 | BLK/BRN | FX102 | RTSI signal

#### Transmission Control Selector Switch

Connector Part Information | F 9-23
--- | ---
Pin | Wire Color | CKT No. | Function
1 | GRN | U900 | Brake to shift signal
2 | BLU | P100 | Sport mode input signal
3-5 | -- | -- | Not used
6 | BLK | F950 F960 | Ground to G103
7 | YEL | B901 | Grounded in PARK
8 | BLK/BRN | FX900 | Sport mode switch signal
9 | YEL | B900 | Gear out of PARK signal