For 1990-2009 cars

Leak Area | Repair Material(s)
--- | ---
Use an equivalent material if necessary.
Bolts, Studs, Screws, and Other Transition Areas | Strip Caulk/3M Thumb Grade Sealer 08578
Cracks and Holes (General, Large) | 3M All Around Autobody Sealant 8500
Cracks and Holes (General, Small) | 3M Drip-Chek Sealer
Drip Moldings | 3M Auto Bedding and Glazing Compound
Joints (Metal) | Brushable/Paintable Seam Sealer
Rear Window | Urethane Adhesive Caulking Kit GM P/N 12346392
Ventilation Ducts | 3M Auto Bedding and Glazing Compound
Weatherstrip Retainers | Foam Tape
Windshield | Urethane Adhesive Caulking Kit GM P/N 12346392