For 1990-2009 cars

#### Interval Switch

Connector Part Information |

• | ZPM 6-55

• | 6-Way M (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-3 | -- | -- | Not used
4 | BLK/YEL | FB3 | Delay Signal
5 | -- | -- | Not used
6 | BLK/WHT | FM99 | Interval Switch On Signal

#### Windshield Washer Nozzle - LH

Connector Part Information |

• | ZPF 2-50

• | 2-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | X2 | B+ from Fuse #14
B | BLK | F2 | Ground to G103

#### Windshield Washer Nozzle - RH

Connector Part Information |

• | ZPF 2-50

• | 2-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | X1 | B+ from Fuse #14
B | BLK | F1 | Ground to G103

#### Windshield Washer Pump

Connector Part Information |

• | ZFW 2-57

• | 2-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/RED | FA80 | Washer Pump Signal
2 | BLK | F30 | Ground to G103

#### Windshield Washer Solvent Level Switch

Connector Part Information |

• | ZPF 2-8

• | 2-Way F (WHT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | F108 | Ground to G103
B | BRN/YEL | XB3 | Low fluid signal

#### Windshield Wiper Motor

Connector Part Information |

• | ZFW 5-3

• | 5-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | B7 | Motor volatage LO Speed
B | BLK | F9 | Ground to G103
C | GRN | U6 | Motor Position Signal
D | BLK/PPL | FY2 | B+ from fuse #9 for wiper position switch
E | WHT | M9 | Motor volatage HI Speed

#### Windshield Wiper Motor Relay K8

Connector Part Information |

• | ZF 9-6

• | 9-Way F (YEL)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/YEL | FB1 | Interval Input signal
2 | BLU | P2 | Output voltage for WSW motor Interval, Mist and Park
3 | -- | -- | Not used
4 | BLK | F10 | Ground to G103
5 | GRN | U10 | Wiper Position Signal
6 | BLK/RED | FA1 | Mist signal
7 | -- | -- | Not used
8 | BLK/PPL | FY1 | B+ from fuse #9
9 | -- | -- | Not used

#### Windshield Wiper and Windshield Washer Switch

Connector Part Information |

• | ZF 9-3

• | 9-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not used
2 | WHT | M9 | WSW motor high voltage
WHT | M808 | WSW motor high voltage
3 | BLK/RED | FA4 | WSW mist signal
4 | BLK/PPL | FY11 | B+ from fuse #9
5 | YEL | B7 | WSW motor low voltage
YEL | B810 | WSW motor low voltage
6-7 | -- | -- | Not used
8 | BLU | P2 | Voltage from WSW relay, for WSW Motor in Mist, Interval and Park
9 | BLK/WHT | FM99 | Interval switch signal