For 1990-2009 cars

Causes | Action
--- | ---
The Selector Lever is in a Position 3. | Adjust the Selector Lever Position Switch/Shift Linkage.
The Selector Lever Position Switch/Shift Linkage is an incorrectly adjusted. | Refer to DTC P0753 1-2/3-4 Shift Solenoid Circuit Electrical .
The Solenoid Valve for the 1-2/3-4 Shift or the On-Off Valve in the Valve Body Assembly is defective. |

1. Search for the defective part.
2. Replace the defective part.

Loss of the hydraulic fluid in Clutch C4 or in the fluid circuit |

1. Search for the leaking part.
2. Replace the leaking part.