For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Seat Shoulder Belt to Guide Adjuster Bolt | 10 N·m | 89 lb in
Right and/or Left Front Seat Belt Guide Screws | 10 N·m | 89 lb in
Right and/or Left Front Seat Retractor Bolt | 35 N·m | 26 lb ft
Right and/or Left Front Seat Retractor Lower Bolt | 35 N·m | 26 lb ft
Right and/or Left Front Seat Shoulder Belt Guide Adjuster Bolts | 35 N·m | 26 lb ft
Rear Seat Belt Buckle Bolt | 35 N·m | 26 lb ft
Rear Seat Belt Retractor Bolt | 35 N·m | 26 lb ft
Rear Seat Belt Center Retractor Bolt | 35 N·m | 26 lb ft
Rear Seat Shoulder Belt Height Adjuster Bolt | 35 N·m | 26 lb ft
Rear Seat Belt with Retractor Belt Lower Belt | 35 N·m | 26 lb ft
Tether Top Strap Anchor Bolt | 20 N·m | 15 lb ft