For 1990-2009 cars

#### Approximate Fluid Capacities

Application | Liters | Gallons | Quarts | Kg | Lb
--- | --- | --- | --- | --- | ---
Air Conditioning (R 134a) | -- | -- | -- | 0.95 | 2
Engine oil (with filter change) | 5.75 | -- | 6.1 | -- | --
Engine oil (without filter change) | 5.5 | -- | 5.8 | -- | --
Fuel Tank | 68.1 | 18 | -- | -- | --
Automatic Transmission (4L30-E) Drain and Refill | 6.6 | -- | 7 | -- | --
Cooling System | 10 | -- | 10.6 | -- | --