For 1990-2009 cars

For the Automatic Day-Night Mirror system, begin the diagnosis by reviewing the system Description and Operation. Reviewing the Description and Operation information will help you determine the correct symptom diagnostic procedure when a malfunction exists. Reviewing the Description and Operation information will also help you determine if the condition described by the customer is normal operation. Refer to Symptoms - Stationary Windows in order to identify the correct procedure for diagnosing the system and where the procedure is located.

For the Rear Window Defogger and Inside Rearview Mirror (w/memory) systems, begin the diagnosis with the Diagnostic System Check - Stationary Windows . The Diagnostic System Check will provide the following information:

• | The identification of the control module(s) which command the system.

• | The ability of the control module(s) to communicate through the serial data circuit.

• | The identification of any stored diagnostic trouble codes (DTCs) and their status.

The use of the Diagnostic System Check will identify the correct procedure for diagnosing the system and where the procedure is located.