For 1990-2009 cars

Illustration | Tool Number/Description
--- | ---
| J 23075 Third Clutch/Servo Piston Spring Compressor
| J 23075-12 Adapter
| J 23080-A Second Clutch Piston Seal Installer
| J 23082-01 Oil Pump Aligner
| J 23085-A Selective Washer Gauge
| J 23129 Universal Seal Remover
| J 23327 Clutch Spring Compressor
| J 23327-90 Fourth Clutch Spring Compressor Adapter
| J 23327-91 Overrun Clutch Spring Compressor Adapter
| J 24773-A Oil Pump Remover
| J 25022 Front End Play Checking Adapter
| J 3289-20 Holding Fixture Base
| J 3387-2 Alignment Pins
| J 36797 Extension Housing Seal Installer
| J 36850 Assembly Lubricant
| J 38428 Servo Piston Ring Installer
| J 38450-A Third Clutch Snap Ring Compressor
| J 38552 Accumulator Cover Remover
| J 38553 3-4 Accumulator Piston Installer
| J 38554 Fourth Clutch Piston Installer
| J 38555-1 Outer Seal Installer
| J 38555-2 Inner Seal Installer
| J 38557 Converter Housing to Pump Assembly Alignment Tool
| J 38559 Compressor
| J 38584 Adapter
| J 38588-1 Guide Pins
| J 6125-1B Slide Hammer
| J 8001 Dial Indicator Set
| J 8059 Snap Ring Pliers
| J 8763-02 Holding Fixture
| 96042102 Turbine Shaft Seal Sizer

Not all of the tools listed require this specific application. If a procedure requires a special tool, the diagnostic procedure will call out the J number. Before you use any tool, first know the tool's abilities and limitations. This knowledge should include the scan tool operation, the proper use of test lights, the jumper wires, and the DVM.

### Scan Tool

For information regarding the use of a particular scan tool, refer to the documentation provided with the tool by the manufacturer. The General Information on the DLC connector, the Serial Data, and the System Diagnostics can be found in Transmission General Information and Engine Controls General Information .

Illustration | Tool Number/Description
--- | ---
| J 39200 High Impedance Multimeter (Digital Voltmeter-DVM)
| Tech II 70000081 Diagnostic Scan Tool
| J 35616-A/BT-8637
| J 35689-A Metri-Pack Terminal Remover
| J 28742-A Weather Pack Terminal Remover
| J 33095/BT-8234-A Control Module Connector Terminal Remover
| J 42250 Terminal Repair Kit
| J 26792/BT-7220-1 Spark Tester
| J 34142-B Unpowered Test Light
| J 42219 Fuel Sender Locknut Wrench
| J 35748 Oil Pressure Sending Unit Socket
| J 23738-A/BT-8512-A Vacuum Pump
| J 39194 Oxygen Sensor Wrench
| J 34730-1A Fuel Pressure Gauge
| J 42242 Fuel Pressure Gauge Adapter
| J 37287-100 Fuel Line Shut-Off Quick Connect Adapters
| J 39021-360 Injector Harness Adapter
| J 37287 Inlet and Return Fuel Line Shut-Off Adapters
| J 39021 Fuel Injector Coil/Balance Tester
| J 41750 EVAP Pressure/Purge Cart
| J 42374 Fuel Line Quick Connect Separators
| J 39021-210 Injector Switch Box
| J 34730-375 Injector Test Light
| J 38522 Variable Signal Generator
| J 38791 Transaxle Test Box
| J 38835 Transmission Jumper Harness (7 Pin)
| J 38791-70 Transmission Test Box Adapter Harness Kit (7 Pin)
| J 38791-80 Transmission Jumper Harness (4 Pin)
| J 38791-90 Transmission Jumper Harness (8 Pin)
| J 35314-A Exhaust Back Pressure Tester
| J 35944-A Oil Cooler and Line Flusher
| J 35944-20 Cooler Flushing Fluid
| J 45096 Transmission Oil Cooling System Flush and Flow Test Tool