For 1990-2009 cars

The PWR SEAT fuse supplies battery voltage to the driver and the passenger seat adjuster switches. Ground is supplied to seat adjuster switch from G103. The seat adjuster switch supplies ground to both sides of the each adjuster motor at all times in both the driver and the passenger seats. Battery voltage is supplied to the appropriate side of each motor when a switch is pressed.