SQUAWK NOISE FROM THE REAR NEW SPRING UPPER INSULATOR. Cadillac Cimarron 1987

For 1990-2009 cars

# SQUAWK NOISE FROM THE REAR NEW SPRING UPPER INSULATOR

#### MODELS AFFECTED: 1982-1988 CIMARRONS

Customers may comment about a squawk or squeak coming from the rear of the vehicle, particularly during cold weather (temperature 40 DEG F or colder). This condition may be caused by distortion of the rear spring upper insulator, resulting in a squeak or squawk noise. This condition may be corrected by installing new rear spring upper insulators, P/N 22555689, followin, the Service Information Manual procedure.

#### IMPORTANT: P/N 22555689 will temporarily be supplied with P/N 10017875 molded into the side. The new part is identified by a white stripe on the edge of the insulator.

Parts are currently available from GMSPO.

For warranty purposes use Labor Operation E5057 at .6 hour.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.